## Sanyo Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x00ff | MakerNoteOffset | int32u |
> 0x0100 | SanyoThumbnail | undef |
> 0x0200 | SpecialMode | int32u[3] |
> 0x0201 | SanyoQuality | int16u |
> 0x0 = Normal/Very Low 0x1 = Normal/Low 0x2 = Normal/Medium Low 0x3 = Normal/Medium 0x4 = Normal/Medium High 0x5 = Normal/High 0x6 = Normal/Very High 0x7 = Normal/Super High 0x100 = Fine/Very Low 0x101 = Fine/Low 0x102 = Fine/Medium Low 0x103 = Fine/Medium 0x104 = Fine/Medium High 0x105 = Fine/High 0x106 = Fine/Very High 0x107 = Fine/Super High 0x200 = Super Fine/Very Low 0x201 = Super Fine/Low 0x202 = Super Fine/Medium Low 0x203 = Super Fine/Medium 0x204 = Super Fine/Medium High 0x205 = Super Fine/High 0x206 = Super Fine/Very High 0x207 = Super Fine/Super High
> 0x0202 | Macro | int16u | 0 = Normal 1 = Macro 2 = View 3 = Manual
> 0x0204 | DigitalZoom | rational64u |
> 0x0207 | SoftwareVersion | Y |
> 0x0208 | PictInfo | Y |
> 0x0209 | CameraID | Y |
> 0x020e | SequentialShot | int16u | 0 = None 1 = Standard 2 = Best 3 = Adjust Exposure
> 0x020f | WideRange | int16u | 0 = Off 1 = On
> 0x0210 | ColorAdjustmentMode | int16u | 0 = Off 1 = On
> 0x0213 | QuickShot | int16u | 0 = Off 1 = On
> 0x0214 | SelfTimer | int16u | 0 = Off 1 = On
> 0x0216 | VoiceMemo | int16u | 0 = Off 1 = On
> 0x0217 | RecordShutterRelease | int16u | 0 = Record while down 1 = Press start, press stop
> 0x0218 | FlickerReduce | int16u | 0 = Off 1 = On
> 0x0219 | OpticalZoomOn | int16u | 0 = Off 1 = On
> 0x021b | DigitalZoomOn | int16u | 0 = Off 1 = On
> 0x021d | LightSourceSpecial | int16u | 0 = Off 1 = On
> 0x021e | Resaved | int16u | 0 = No 1 = Yes
> 0x021f | SceneSelect | int16u |
> 0 = Off 1 = Sport 2 = TV 3 = Night |  | 4 = User 1 5 = User 2 6 = Lamp
> 0x0223 | ManualFocusDistance FaceInfo | rational64u - | Sanyo FaceInfo
> 0x0224 | SequenceShotInterval | int16u | 0 = 5 frames/s 1 = 10 frames/s 2 = 15 frames/s 3 = 20 frames/s
> 0x0225 | FlashMode | int16u | 0 = Auto 1 = Force 2 = Disabled 3 = Red eye
> 0x0e00 | PrintIM | - | --> PrintIM Tags
> 0x0f00 | DataDump | N |

## Sanyo FaceInfo Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FacesDetected | int32u |
> 4 | FacePosition | int32u[4] | (left, top, right and bottom coordinates of detected face in an unrotated 640-pixel-wide image, with increasing Y downwards)

## Sanyo MOV Tags

This information is found in Sanyo MOV videos.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |
> 24 | Model | N |
> 38 | ExposureTime | N |
> 42 | FNumber | N |
> 50 | ExposureCompensation | N |
> 68 | WhiteBalance | N |
> 0 = Auto 1 = Daylight 2 = Shade |  | 3 = Fluorescent 4 = Tungsten 5 = Manual
> 72 | FocalLength | N |

## Sanyo MP4 Tags

This information is found in Sanyo MP4 videos.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |
> 24 | Model | N |
> 50 | FNumber | N |
> 58 | ExposureCompensation | N |
> 106 | ISO | N |
> 209 | Software | N | (these tags are shifted up by 1 byte for some models like the HD1A)
> 210 | Software | N |
> 241 | Thumbnail | - | --> Sanyo Thumbnail Tags
> 242 | Thumbnail | - | --> Sanyo Thumbnail Tags

## Sanyo Thumbnail Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | ThumbnailWidth | N |
> 2 | ThumbnailHeight | N |
> 3 | ThumbnailLength | N |
> 4 | ThumbnailOffset | N |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Nov 22, 2011

<-- ExifTool Tag Names