## NikonCustom Tags

Unfortunately, the NikonCustom settings are stored in a binary data block which changes from model to model. This means that significant effort must be spent in decoding these for each model, usually requiring hundreds of test images from a dedicated Nikon owner. For this reason, the NikonCustom settings have not been decoded for all models. The tables below list the custom settings for the currently supported models.

## NikonCustom SettingsD40 Tags

Custom settings for the Nikon D40.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | Beep | int8u | [val >> 7 & 0x1] 0 = On 1 = Off
> 0.2 | AFAssist | int8u | [val >> 6 & 0x1] 0 = On 1 = Off
> 0.3 | NoMemoryCard | int8u | [val >> 5 & 0x1] 0 = Release Locked 1 = Enable Release
> 0.4 | ImageReview | int8u | [val >> 4 & 0x1] 0 = On 1 = Off
> 1.1 | AutoISO | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 1.2 | AutoISOMax | int8u | [val >> 4 & 0x3] 1 = 400 2 = 800 3 = 1600
> 1.3 | AutoISOMinShutterSpeed | int8u | [val & 0x7]
> 0 = 1/125 s 1 = 1/60 s 2 = 1/30 s 3 = 1/15 s |  | 4 = 1/8 s 5 = 1/4 s 6 = 1/2 s 7 = 1 s
> 2.1 | ImageReviewTime | int8u | [val & 0x7] 0 = 4 s 1 = 8 s 2 = 20 s 3 = 1 min 4 = 10 min
> 3.1 | MonitorOffTime | int8u | [val >> 5 & 0x7] 0 = 4 s 1 = 8 s 2 = 20 s 3 = 1 min 4 = 10 min
> 3.2 | MeteringTime | int8u | [val >> 2 & 0x7] 0 = 4 s 1 = 8 s 2 = 20 s 3 = 1 min 4 = 30 min
> 3.3 | SelfTimerTime | int8u | [val & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 3.4 | RemoteOnDuration | int8u | [val >> 6 & 0x3] 0 = 1 min 1 = 5 min 2 = 10 min 3 = 15 min
> 4.1 | AELockButton | int8u | [val >> 1 & 0x7] 0 = AE/AF Lock 1 = AE Lock Only 2 = AF Lock Only 3 = AE Lock (hold) 4 = AF-ON
> 4.2 | AELock | int8u | [val & 0x1] 0 = Off 1 = On
> 5.1 | ShootingModeSetting | int8u | [val >> 4 & 0x7] 0 = Single Frame 1 = Continuous 2 = Self-timer 3 = Delayed Remote 4 = Quick-response Remote
> 5.2 | TimerFunctionButton | int8u | [val & 0x7] 0 = Shooting Mode 1 = Image Quality/Size 2 = ISO 3 = White Balance 4 = Self-timer
> 6.1 | Metering | int8u | [val & 0x3] 0 = Matrix 1 = Center-weighted 2 = Spot
> 8.1 | InternalFlash | int8u | [val >> 4 & 0x1] 0 = TTL 1 = Manual
> 8.2 | ManualFlashOutput | int8u | [val & 0x7]
> 9 | FlashLevel | int8s |
> 10.1 | FocusModeSetting | int8u | [val >> 6 & 0x3] 0 = Manual 1 = AF-S 2 = AF-C 3 = AF-A
> 11.1 | AFAreaModeSetting | int8u | [val >> 4 & 0x3] 0 = Single Area 1 = Dynamic Area 2 = Closest Subject

## NikonCustom SettingsD80 Tags

Custom settings for the Nikon D80.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | Beep | int8u | [val >> 7 & 0x1] 0 = On 1 = Off
> 0.2 | AFAssist | int8u | [val >> 6 & 0x1] 0 = On 1 = Off
> 0.3 | NoMemoryCard | int8u | [val >> 5 & 0x1] 0 = Release Locked 1 = Enable Release
> 0.4 | ImageReview | int8u | [val >> 4 & 0x1] 0 = On 1 = Off
> 0.5 | Illumination | int8u | [val >> 3 & 0x1] 0 = Off 1 = On
> 0.6 | MainDialExposureComp | int8u | [val >> 2 & 0x1] 0 = Off 1 = On
> 0.7 | EVStepSize | int8u | [val & 0x1] 0 = 1/3 EV 1 = 1/2 EV
> 1.1 | AutoISO | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 1.2 | AutoISOMax | int8u | [val >> 4 & 0x3] 0 = 200 1 = 400 2 = 800 3 = 1600
> 1.3 | AutoISOMinShutterSpeed | int8u | [val & 0xf]
> 0 = 1/125 s 1 = 1/100 s 2 = 1/80 s 3 = 1/60 s 4 = 1/40 s 5 = 1/30 s |  | 6 = 1/15 s 7 = 1/8 s 8 = 1/4 s 9 = 1/2 s 10 = 1 s
> 2.1 | AutoBracketSet | int8u | [val >> 6 & 0x3] 0 = AE & Flash 1 = AE Only 2 = Flash Only 3 = WB Bracketing
> 2.2 | AutoBracketOrder | int8u | [val >> 5 & 0x1] 0 = 0,-,+ 1 = -,0,+
> 3.1 | MonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 5 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 3.2 | MeteringTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 1 = 6 s 2 = 8 s |  | 3 = 16 s 4 = 30 s 5 = 30 min
> 3.3 | SelfTimerTime | int8u | [val & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 4.1 | AELockButton | int8u | [val >> 1 & 0xf]
> 0 = AE/AF Lock 1 = AE Lock Only 2 = AF Lock Only 3 = AE Lock (hold) 4 = AF-ON 5 = FV Lock 6 = Focus Area Selection 7 = AE-L/AF-L/AF Area 8 = AE-L/AF Area 9 = AF-L/AF Area 10 = AF-ON/AF Area
> 4.2 | AELock | int8u | [val & 0x1] 0 = Off 1 = On
> 4.3 | RemoteOnDuration | int8u | [val >> 6 & 0x3] 0 = 1 min 1 = 5 min 2 = 10 min 3 = 15 min
> 5.1 | CommandDials | int8u | [val >> 7 & 0x1] 0 = Standard (Main Shutter, Sub Aperture) 1 = Reversed (Main Aperture, Sub Shutter)
> 5.2 | FunctionButton | int8u | [val >> 3 & 0xf]
> 0 = ISO Display 1 = Framing Grid 2 = AF-area Mode 3 = Center AF Area 4 = FV Lock |  | 5 = Flash Off 6 = Matrix Metering 7 = Center-weighted 8 = Spot Metering
> 6.1 | GridDisplay | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 6.2 | ViewfinderWarning | int8u | [val >> 6 & 0x1] 0 = On 1 = Off
> 6.3 | CenterWeightedAreaSize | int8u | [val >> 2 & 0x3] 0 = 6 mm 1 = 8 mm 2 = 10 mm
> 6.4 | ExposureDelayMode | int8u | [val >> 5 & 0x1] 0 = Off 1 = On
> 6.5 | MB-D80Batteries | int8u | [val & 0x3] 0 = LR6 (AA Alkaline) 1 = HR6 (AA Ni-MH) 2 = FR6 (AA Lithium) 3 = ZR6 (AA Ni-Mg)
> 7.1 | FlashWarning | int8u | [val >> 7 & 0x1] 0 = On 1 = Off
> 7.2 | FlashShutterSpeed | int8u | [val >> 3 & 0xf]
> 7.3 | AutoFP | int8u | [val >> 2 & 0x1] 0 = Off 1 = On
> 7.4 | ModelingFlash | int8u | [val >> 1 & 0x1] 0 = Off 1 = On
> 8.1 | InternalFlash | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Manual 2 = Repeating Flash 3 = Commander Mode
> 8.2 | ManualFlashOutput | int8u | [val & 0x7]
> 9.1 | RepeatingFlashOutput | int8u | [val >> 4 & 0x7]
> 9.2 | RepeatingFlashCount | int8u | [val & 0xf]
> 10.1 | RepeatingFlashRate | int8u | [val >> 4 & 0xf]
> 10.2 | CommanderChannel | int8u | [val & 0x3]
> 11.1 | CommanderInternalFlash | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Manual 2 = Off
> 11.2 | CommanderGroupAMode | int8u | [val >> 4 & 0x3] 0 = TTL 1 = Auto Aperture 2 = Manual 3 = Off
> 11.3 | CommanderGroupBMode | int8u | [val >> 2 & 0x3] 0 = TTL 1 = Auto Aperture 2 = Manual 3 = Off
> 12.1 | CommanderInternalTTLComp | int8u | [val & 0x1f]
> 12.2 | CommanderInternalManualOutput | int8u | [val >> 5 & 0x7]
> 13.1 | CommanderGroupA_TTL-AAComp | int8u | [val & 0x1f]
> 13.2 | CommanderGroupAManualOutput | int8u | [val >> 5 & 0x7]
> 14.1 | CommanderGroupB_TTL-AAComp | int8u | [val & 0x1f]
> 14.2 | CommanderGroupBManualOutput | int8u | [val >> 5 & 0x7]
> 15.1 | CenterAFArea | int8u | [val >> 7 & 0x1] 0 = Normal Zone 1 = Wide Zone
> 15.2 | FocusAreaSelection | int8u | [val >> 2 & 0x1] 0 = No Wrap 1 = Wrap
> 15.3 | AFAreaIllumination | int8u | [val & 0x3] 0 = Auto 1 = Off 2 = On
> 16.1 | AFAreaModeSetting | int8u | [val >> 6 & 0x3] 0 = Single Area 1 = Dynamic Area 2 = Auto-area

## NikonCustom SettingsD90 Tags

Custom settings for the D90.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | LightSwitch | int8u | [val >> 3 & 0x1] 0 = LCD Backlight 1 = LCD Backlight and Shooting Information
> 2.1 | AFAreaModeSetting | int8u | [val >> 5 & 0x3] 0 = Single Area 1 = Dynamic Area 2 = Auto-area 3 = 3D-tracking (11 points)
> 2.2 | CenterFocusPoint | int8u | [val >> 4 & 0x1] 0 = Normal Zone 1 = Wide Zone
> 2.3 | AFAssist | int8u | [val & 0x1] 0 = On 1 = Off
> 2.4 | AFPointIllumination | int8u | [val >> 1 & 0x3] 0 = Auto 1 = On 2 = Off
> 2.5 | FocusPointWrap | int8u | [val >> 3 & 0x1] 0 = No Wrap 1 = Wrap
> 3.1 | AELockForMB-D80 | int8u | [val >> 2 & 0x7]
> 0 = AE Lock Only 1 = AF Lock Only 2 = AE Lock (hold) 3 = AF-On 4 = FV Lock 5 = Focus Point Selection 7 = AE/AF Lock
> 3.2 | MB-D80BatteryType | int8u | [val & 0x3] 0 = LR6 (AA alkaline) 1 = HR6 (AA Ni-MH) 2 = FR6 (AA lithium) 3 = ZR6 (AA Ni-Mn)
> 4.1 | Beep | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 4.2 | GridDisplay | int8u | [val >> 1 & 0x1] 0 = Off 1 = On
> 4.3 | ISODisplay | int8u | [val >> 2 & 0x3] 0 = Show ISO/Easy ISO 1 = Show ISO Sensitivity 3 = Show Frame Count
> 4.4 | ViewfinderWarning | int8u | [val & 0x1] 0 = On 1 = Off
> 4.5 | NoMemoryCard | int8u | [val >> 5 & 0x1] 0 = Release Locked 1 = Enable Release
> 5.1 | ScreenTips | int8u | [val >> 2 & 0x1] 0 = Off 1 = On
> 5.2 | FileNumberSequence | int8u | [val >> 3 & 0x1] 0 = On 1 = Off
> 5.3 | ShootingInfoDisplay | int8u | [val >> 6 & 0x3] 0 = Auto 2 = Manual (dark on light) 3 = Manual (light on dark)
> 5.4 | LCDIllumination | int8u | [val >> 5 & 0x1] 0 = Off 1 = On
> 6.1 | EasyExposureComp | int8u | [val & 0x1] 0 = Off 1 = On
> 6.2 | ReverseIndicators | int8u | [val >> 7 & 0x1] 0 = + 0 - 1 = - 0 +
> 7.1 | ExposureControlStepSize | int8u | [val >> 6 & 0x1] 0 = 1/3 EV 1 = 1/2 EV
> 8.1 | CenterWeightedAreaSize | int8u | [val >> 5 & 0x3] 0 = 6 mm 1 = 8 mm 2 = 10 mm
> 8.2 | FineTuneOptMatrixMetering | int8u | [val & 0xf]
> 9.1 | FineTuneOptCenterWeighted | int8u | [val >> 4 & 0xf]
> 9.2 | FineTuneOptSpotMetering | int8u | [val & 0xf]
> 11.1 | CLModeShootingSpeed | int8u | [val & 0x7]
> 11.2 | ExposureDelayMode | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 13.1 | AutoBracketSet | int8u | [val >> 5 & 0x7] 0 = AE & Flash 1 = AE Only 2 = Flash Only 3 = WB Bracketing 4 = Active D-Lighting
> 13.2 | AutoBracketOrder | int8u | [val >> 4 & 0x1] 0 = 0,-,+ 1 = -,0,+
> 14.1 | FuncButton | int8u | [val >> 3 & 0xf]
> 1 = Framing Grid 2 = AF-area Mode 3 = Center Focus Point 4 = FV Lock 5 = Flash Off 6 = Matrix Metering 7 = Center-weighted Metering 8 = Spot Metering 9 = My Menu Top 10 = + NEF (RAW)
> 16.1 | OKButton | int8u | [val >> 3 & 0x3] 0 = Not Used 1 = Select Center Focus Point 2 = Highlight Active Focus Point 3 = Not Used
> 17.1 | AELockButton | int8u | [val >> 3 & 0x7]
> 0 = AE/AF Lock 1 = AE Lock Only 2 = AF Lock Only |  | 3 = AE Lock (hold) 4 = AF-ON 5 = FV Lock
> 18.1 | CommandDialsReverseRotation | int8u | [val >> 7 & 0x1] 0 = No 1 = Yes
> 18.2 | ShutterReleaseButtonAE-L | int8u | [val >> 1 & 0x1] 0 = Off 1 = On
> 19.1 | MeteringTime | int8u | [val >> 4 & 0xf]
> 0 = 4 s 1 = 6 s 2 = 8 s 3 = 16 s 4 = 30 s |  | 5 = 1 min 6 = 5 min 7 = 10 min 8 = 30 min
> 19.2 | RemoteOnDuration | int8u | [val & 0x3] 0 = 1 min 1 = 5 min 2 = 10 min 3 = 15 min
> 20.1 | SelfTimerTime | int8u | [val >> 6 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 20.2 | SelfTimerShotCount | int8u | [val >> 1 & 0xf]
> 21.1 | PlaybackMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 21.2 | ImageReviewTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 22.1 | MenuMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 22.2 | ShootingInfoMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 23.1 | FlashShutterSpeed | int8u | [val & 0xf]
> 0 = 1/60 s 1 = 1/30 s 2 = 1/15 s 3 = 1/8 s 4 = 1/4 s 5 = 1/2 s |  | 6 = 1 s 7 = 2 s 8 = 4 s 9 = 8 s 10 = 15 s 11 = 30 s
> 24.1 | InternalFlash | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Manual 2 = Repeating Flash 3 = Commander Mode
> 24.2 | ManualFlashOutput | int8u | [val & 0x1f]
> 25.1 | RepeatingFlashOutput | int8u | [val >> 4 & 0x7]
> 25.2 | RepeatingFlashCount | int8u | [val & 0xf]
> 26.1 | RepeatingFlashRate | int8u | [val >> 4 & 0xf]
> 31.1 | FlashWarning | int8u | [val >> 7 & 0x1] 0 = On 1 = Off
> 31.2 | CommanderInternalTTLComp | int8u | [val & 0x1f]
> 31.3 | ModelingFlash | int8u | [val >> 5 & 0x1] 0 = On 1 = Off
> 31.4 | AutoFP | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 32.1 | CommanderGroupA_TTLComp | int8u | [val & 0x1f]
> 33.1 | CommanderGroupB_TTLComp | int8u | [val & 0x1f]
> 34.1 | LiveViewAF | int8u | [val >> 6 & 0x3] 0 = Face Priority 1 = Wide Area 2 = Normal Area

## NikonCustom SettingsD3 Tags

Custom settings for the D3, D3S, D3X, D300 and D300S.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | CustomSettingsBank | int8u | [val & 0x3] 0 = A 1 = B 2 = C 3 = D
> 0.2 | CustomSettingsAllDefault | int8u | ("No" if any custom setting for this bank was changed from the default) [val >> 7 & 0x1] 0 = Yes 1 = No
> 1.1 | AF-CPrioritySelection | int8u | [val >> 6 & 0x3] 0 = Release 1 = Release + Focus 2 = Focus
> 1.2 | AF-SPrioritySelection | int8u | [val >> 5 & 0x1] 0 = Focus 1 = Release
> 1.3 | AFPointSelection | int8u | [val >> 4 & 0x1] 0 = 51 Points 1 = 11 Points
> 1.4 | DynamicAFArea | int8u | [val >> 2 & 0x3] 0 = 9 Points 1 = 21 Points 2 = 51 Points 3 = 51 Points (3D-tracking)
> 1.5 | FocusTrackingLockOn | int8u | (not D3S) [val & 0x3] 0 = Long 1 = Normal 2 = Short 3 = Off
> 2.1 | AFActivation | int8u | [val >> 7 & 0x1] 0 = Shutter/AF-On 1 = AF-On Only
> 2.2 | FocusPointWrap | int8u | [val >> 3 & 0x1] 0 = No Wrap 1 = Wrap
> 2.3 | AFPointIllumination | int8u | (D3) [val >> 5 & 0x3] 0 = On in Continuous Shooting and Manual Focusing 1 = On During Manual Focusing 2 = On in Continuous Shooting Modes 3 = Off (D300) [val >> 1 & 0x3] 0 = Auto 1 = Off 2 = On
> 2.4 | AFPointBrightness | int8u | (D3 only) [val >> 1 & 0x3] 0 = Low 1 = Normal 2 = High 3 = Extra High
> 2.5 | AFAssist | int8u | (D300 only) [val & 0x1] 0 = On 1 = Off
> 3.1 | AFOnButton | int8u | (D3 only) [val & 0x7]
> 0 = AF On 1 = AE/AF Lock 2 = AE Lock Only 3 = AE Lock (reset on release) 4 = AE Lock (hold) 5 = AF Lock Only
> 3.2 | VerticalAFOnButton | int8u | (D3 only) [val >> 4 & 0x7]
> 0 = AF On 1 = AE/AF Lock 2 = AE Lock Only 3 = AE Lock (reset on release) 4 = AE Lock (hold) 5 = AF Lock Only 7 = Same as AF On
> 3.3 | AF-OnForMB-D10 | int8u | (D300 only) [val >> 4 & 0x7]
> 0 = AF-On 1 = AE/AF Lock 2 = AE Lock Only 3 = AE Lock (reset on release) 4 = AE Lock (hold) 5 = AF Lock Only 6 = Same as FUNC Button
> 4.1 | FocusTrackingLockOn | int8u | (D3S only) [val & 0x7]
> 0 = 5 (Long) 1 = 4 2 = 3 (Normal) |  | 3 = 2 4 = 1 (Short) 5 = Off
> 4.2 | AssignBktButton | int8u | (D3S only) [val >> 3 & 0x1] 0 = Auto Bracketing 1 = Multiple Exposure
> 4.3 | MultiSelectorLiveView | int8u | (D3S only) [val >> 6 & 0x3] 0 = Reset 1 = Zoom On/Off 2 = Start Movie Recording 3 = Not Used
> 4.4 | InitialZoomLiveView | int8u | (D3S only) [val >> 4 & 0x3] 0 = Low Magnification 1 = Medium Magnification 2 = High Magnification
> 6.1 | ISOStepSize | int8u | [val >> 6 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 6.2 | ExposureControlStepSize | int8u | [val >> 4 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 6.3 | ExposureCompStepSize | int8u | [val >> 2 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 6.4 | EasyExposureCompensation | int8u | [val & 0x3] 0 = Off 1 = On 2 = On (auto reset)
> 7.1 | CenterWeightedAreaSize | int8u | (D3) [val >> 5 & 0x7] 0 = 8 mm 1 = 12 mm 2 = 15 mm 3 = 20 mm 4 = Average (D300) [val >> 5 & 0x7] 0 = 6 mm 1 = 8 mm 2 = 10 mm 3 = 13 mm 4 = Average
> 7.2 | FineTuneOptCenterWeighted | int8u | [val & 0xf]
> 8.1 | FineTuneOptMatrixMetering | int8u | [val >> 4 & 0xf]
> 8.2 | FineTuneOptSpotMetering | int8u | [val & 0xf]
> 9.1 | MultiSelectorShootMode | int8u | [val >> 6 & 0x3] 0 = Select Center Focus Point 1 = Highlight Active Focus Point 2 = Not Used
> 9.2 | MultiSelectorPlaybackMode | int8u | (all models except D3S) [val >> 4 & 0x3] 0 = Thumbnail On/Off 1 = View Histograms 2 = Zoom On/Off 3 = Choose Folder
> 9.3 | InitialZoomSetting | int8u | (D3) [val >> 2 & 0x3] 0 = High Magnification 1 = Medium Magnification 2 = Low Magnification (D300) [val >> 2 & 0x3] 0 = Low Magnification 1 = Medium Magnification 2 = High Magnification
> 9.4 | MultiSelector | int8u | [val & 0x1] 0 = Do Nothing 1 = Reset Meter-off Delay
> 10.1 | ExposureDelayMode | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 10.2 | CLModeShootingSpeed | int8u | [val & 0x7]
> 10.3 | CHModeShootingSpeed | int8u | (D3 only) [val >> 4 & 0x3] 0 = 9 fps 1 = 10 fps 2 = 11 fps
> 11 | MaxContinuousRelease | int8u |
> 12.1 | ReverseIndicators | int8u | [val >> 5 & 0x1] 0 = + 0 - 1 = - 0 +
> 12.2 | FileNumberSequence | int8u | (D3) [val >> 1 & 0x1] 0 = On 1 = Off (D300) [val >> 3 & 0x1] 0 = On 1 = Off
> 12.3 | RearDisplay | int8u | (D3 only) [val >> 7 & 0x1] 0 = ISO 1 = Exposures Remaining
> 12.4 | ViewfinderDisplay | int8u | (D3 only) [val >> 6 & 0x1] 0 = Frame Count 1 = Exposures Remaining
> 12.5 | BatteryOrder | int8u | (D300 only) [val >> 2 & 0x1] 0 = MB-D10 First 1 = Camera Battery First
> 12.6 | MB-D10Batteries | int8u | (D300 only) [val & 0x3] 0 = LR6 (AA alkaline) 1 = HR6 (AA Ni-MH) 2 = FR6 (AA lithium) 3 = ZR6 (AA Ni-Mn)
> 12.7 | ScreenTips | int8u | [val >> 4 & 0x1] 0 = On 1 = Off
> 13.1 | Beep | int8u | [val >> 6 & 0x3] 0 = High 1 = Low 2 = Off
> 13.2 | ShootingInfoDisplay | int8u | [val >> 4 & 0x3] 0 = Auto 1 = Auto 2 = Manual (dark on light) 3 = Manual (light on dark)
> 13.3 | GridDisplay | int8u | (D300 only) [val >> 1 & 0x1] 0 = Off 1 = On
> 13.4 | ViewfinderWarning | int8u | (D300 only) [val & 0x1] 0 = On 1 = Off
> 13.5 | MultiSelectorPlaybackMode | int8u | (D3S only) [val & 0x3] 0 = Thumbnail On/Off 1 = View Histograms 2 = Zoom On/Off
> 14.1 | PreviewButton FuncButton | int8u int8u | (D3) [val >> 3 & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = Flash Off 9 = Bracketing Burst 10 = Matrix Metering 11 = Center-weighted Metering 12 = Spot Metering 13 = Virtual Horizon 15 = Playback 16 = My Menu Top
> (D300) [val >> 3 & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 9 = Flash Off 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top 16 = + NEF (RAW)
> 14.2 | PreviewButtonPlusDials FuncButtonPlusDials | int8u int8u | (D3) [val & 0x7]
> 0 = None 1 = Choose Image Area (FX/DX/5:4) 2 = One Step Speed/Aperture 3 = Choose Non-CPU Lens Number 5 = Choose Image Area (FX/DX) 6 = Shooting Bank Menu 7 = Dynamic AF Area
> (D300) [val & 0x7] 0 = None 2 = One Step Speed/Aperture 3 = Choose Non-CPU Lens Number 5 = Auto Bracketing 6 = Dynamic AF Area
> 15.1 | FuncButton PreviewButton | int8u int8u | (D3) [val >> 3 & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = Flash Off 9 = Bracketing Burst 10 = Matrix Metering 11 = Center-weighted Metering 12 = Spot Metering 13 = Virtual Horizon 15 = Playback 16 = My Menu Top
> (D300) [val >> 3 & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 9 = Flash Off 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top 16 = + NEF (RAW)
> 15.2 | FuncButtonPlusDials PreviewButtonPlusDials | int8u int8u | (D3) [val & 0x7]
> 0 = None 1 = Choose Image Area (FX/DX/5:4) 2 = One Step Speed/Aperture 3 = Choose Non-CPU Lens Number 4 = Focus Point Selection 5 = Choose Image Area (FX/DX) 6 = Shooting Bank Menu 7 = Dynamic AF Area
> (D300) [val & 0x7] 0 = None 2 = One Step Speed/Aperture 3 = Choose Non-CPU Lens Number 5 = Auto Bracketing 6 = Dynamic AF Area
> 16.1 | AELockButton | int8u | (D3) [val >> 3 & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = Flash Off 9 = Bracketing Burst 10 = Matrix Metering 11 = Center-weighted Metering 12 = Spot Metering 13 = Virtual Horizon 14 = AF On 15 = Playback 16 = My Menu Top
> (D300) [val >> 3 & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF On 9 = Flash Off 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top 16 = + NEF (RAW)
> 16.2 | AELockButtonPlusDials | int8u | (D3) [val & 0x7]
> 0 = None 1 = Choose Image Area (FX/DX/5:4) 2 = One Step Speed/Aperture 3 = Choose Non-CPU Lens Number 5 = Choose Image Area (FX/DX) 6 = Shooting Bank Menu 7 = Dynamic AF Area
> (D300) [val & 0x7] 0 = None 3 = Choose Non-CPU Lens Number 5 = Auto Bracketing 6 = Dynamic AF Area
> 17.1 | CommandDialsReverseRotation | int8u | [val >> 7 & 0x1] 0 = No 1 = Yes
> 17.2 | CommandDialsChangeMainSub | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 17.3 | CommandDialsApertureSetting | int8u | [val >> 5 & 0x1] 0 = Sub-command Dial 1 = Aperture Ring
> 17.4 | CommandDialsMenuAndPlayback | int8u | [val >> 4 & 0x1] 0 = Off 1 = On
> 17.5 | LCDIllumination | int8u | [val >> 3 & 0x1] 0 = Off 1 = On
> 17.6 | PhotoInfoPlayback | int8u | [val >> 2 & 0x1] 0 = Info Up-down, Playback Left-right 1 = Info Left-right, Playback Up-down
> 17.7 | ShutterReleaseButtonAE-L | int8u | [val >> 1 & 0x1] 0 = Off 1 = On
> 17.8 | ReleaseButtonToUseDial | int8u | [val & 0x1] 0 = No 1 = Yes
> 18.1 | SelfTimerTime | int8u | [val >> 3 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 18.2 | MonitorOffTime | int8u | [val & 0x7] 0 = 10 s 1 = 20 s 2 = 1 min 3 = 5 min 4 = 10 min
> 20.1 | FlashSyncSpeed | int8u | (D3) [val >> 5 & 0x7]
> 0 = 1/250 s (auto FP) 1 = 1/250 s 2 = 1/200 s 3 = 1/160 s |  | 4 = 1/125 s 5 = 1/100 s 6 = 1/80 s 7 = 1/60 s
> (D300) [val >> 4 & 0xf]
> 0 = 1/320 s (auto FP) 1 = 1/250 s (auto FP) 2 = 1/250 s 3 = 1/200 s 4 = 1/160 s |  | 5 = 1/125 s 6 = 1/100 s 7 = 1/80 s 8 = 1/60 s
> 20.2 | FlashShutterSpeed | int8u | [val & 0xf]
> 0 = 1/60 s 1 = 1/30 s 2 = 1/15 s 3 = 1/8 s 4 = 1/4 s 5 = 1/2 s |  | 6 = 1 s 7 = 2 s 8 = 4 s 9 = 8 s 10 = 15 s 11 = 30 s
> 21.1 | AutoBracketSet | int8u | (D3 and D300) [val >> 6 & 0x3] 0 = AE & Flash 1 = AE Only 2 = Flash Only 3 = WB Bracketing (D3S and D300S) [val >> 5 & 0x7] 0 = AE & Flash 1 = AE Only 2 = Flash Only 3 = WB Bracketing 4 = ADL Bracketing
> 21.2 | AutoBracketModeM | int8u | (D3 and D300) [val >> 4 & 0x3] 0 = Flash/Speed 1 = Flash/Speed/Aperture 2 = Flash/Aperture 3 = Flash Only (D3S and D300S) [val >> 3 & 0x3] 0 = Flash/Speed 1 = Flash/Speed/Aperture 2 = Flash/Aperture 3 = Flash Only
> 21.3 | AutoBracketOrder | int8u | (D3 and D300) [val >> 3 & 0x1] 0 = 0,-,+ 1 = -,0,+ (D3S and D300S) [val >> 2 & 0x1] 0 = 0,-,+ 1 = -,0,+
> 21.4 | ModelingFlash | int8u | [val & 0x1] 0 = On 1 = Off
> 22.1 | NoMemoryCard | int8u | [val >> 7 & 0x1] 0 = Release Locked 1 = Enable Release
> 22.2 | MeteringTime | int8u | [val & 0xf]
> 0 = 4 s 1 = 6 s 2 = 8 s 3 = 16 s 4 = 30 s |  | 5 = 1 min 6 = 5 min 7 = 10 min 8 = 30 min 9 = No Limit
> 23.1 | InternalFlash | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Manual 2 = Repeating Flash 3 = Commander Mode
> 25.1 | ImageReviewTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 25.2 | PlaybackMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 26.1 | MenuMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 26.2 | ShootingInfoMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min

## NikonCustom SettingsD700 Tags

Custom settings for the D700.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | CustomSettingsBank | int8u | [val & 0x3] 0 = A 1 = B 2 = C 3 = D
> 0.2 | CustomSettingsAllDefault | int8u | ("No" if any custom setting for this bank was changed from the default) [val >> 7 & 0x1] 0 = Yes 1 = No
> 1.1 | AF-CPrioritySelection | int8u | [val >> 6 & 0x3] 0 = Release 1 = Release + Focus 2 = Focus
> 1.2 | AF-SPrioritySelection | int8u | [val >> 5 & 0x1] 0 = Focus 1 = Release
> 1.3 | AFPointSelection | int8u | [val >> 4 & 0x1] 0 = 51 Points 1 = 11 Points
> 1.4 | DynamicAFArea | int8u | [val >> 2 & 0x3] 0 = 9 Points 1 = 21 Points 2 = 51 Points 3 = 51 Points (3D-tracking)
> 2.1 | AFActivation | int8u | [val >> 7 & 0x1] 0 = Shutter/AF-On 1 = AF-On Only
> 2.2 | FocusPointWrap | int8u | [val >> 3 & 0x1] 0 = No Wrap 1 = Wrap
> 2.3 | AFPointIllumination | int8u | [val >> 1 & 0x3] 0 = Auto 1 = Off 2 = On
> 2.4 | AFAssist | int8u | [val & 0x1] 0 = On 1 = Off
> 3.1 | FocusTrackingLockOn | int8u | [val & 0x7]
> 0 = 3 Normal 1 = 4 2 = 5 Long |  | 3 = 2 4 = 1 Short 5 = Off
> 3.2 | AF-OnForMB-D10 | int8u | [val >> 4 & 0x7]
> 0 = AF-On 1 = AE/AF Lock 2 = AE Lock Only 3 = AE Lock (reset on release) 4 = AE Lock (hold) 5 = AF Lock Only 6 = Same as FUNC Button
> 4.1 | ISOStepSize | int8u | [val >> 6 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 4.2 | ExposureControlStepSize | int8u | [val >> 4 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 4.3 | ExposureCompStepSize | int8u | [val >> 2 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 4.4 | EasyExposureCompensation | int8u | [val & 0x3] 0 = Off 1 = On 2 = On (auto reset)
> 5.1 | CenterWeightedAreaSize | int8u | [val >> 4 & 0x7] 0 = 8 mm 1 = 12 mm 2 = 15 mm 3 = 20 mm 4 = Average
> 6.1 | FineTuneOptMatrixMetering | int8u | [val >> 4 & 0xf]
> 6.2 | FineTuneOptSpotMetering | int8u | [val & 0xf]
> 7.1 | ShutterReleaseButtonAE-L | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 7.2 | SelfTimerTime | int8u | [val >> 4 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 7.3 | MeteringTime | int8u | [val & 0xf]
> 0 = 4 s 1 = 6 s 2 = 8 s 3 = 16 s 4 = 30 s |  | 5 = 1 min 6 = 5 min 7 = 10 min 8 = 30 min 9 = No Limit
> 8.1 | PlaybackMonitorOffTime | int8u | [val >> 3 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 8.2 | MenuMonitorOffTime | int8u | [val & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 9.1 | ShootingInfoMonitorOffTime | int8u | [val >> 3 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 9.2 | ImageReviewTime | int8u | [val & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 10.1 | Beep | int8u | [val >> 6 & 0x3] 0 = High 1 = Low 2 = Off
> 10.2 | ShootingInfoDisplay | int8u | [val >> 4 & 0x3] 0 = Auto 1 = Auto 2 = Manual (dark on light) 3 = Manual (light on dark)
> 10.3 | LCDIllumination | int8u | [val >> 3 & 0x1] 0 = Off 1 = On
> 10.4 | ExposureDelayMode | int8u | [val >> 2 & 0x1] 0 = Off 1 = On
> 10.5 | GridDisplay | int8u | [val >> 1 & 0x1] 0 = Off 1 = On
> 11.1 | FileNumberSequence | int8u | [val >> 6 & 0x1] 0 = On 1 = Off
> 11.2 | CLModeShootingSpeed | int8u | [val & 0x7]
> 12 | MaxContinuousRelease | int8u |
> 13.1 | ScreenTips | int8u | [val >> 3 & 0x1] 0 = On 1 = Off
> 13.2 | BatteryOrder | int8u | [val >> 2 & 0x1] 0 = MB-D10 First 1 = Camera Battery First
> 13.3 | MB-D10BatteryType | int8u | [val & 0x3] 0 = LR6 (AA alkaline) 1 = HR6 (AA Ni-MH) 2 = FR6 (AA lithium) 3 = ZR6 (AA Ni-Mn)
> 15.1 | FlashSyncSpeed | int8u | [val >> 4 & 0xf]
> 0 = 1/320 s (auto FP) 1 = 1/250 s (auto FP) 2 = 1/250 s 3 = 1/200 s 4 = 1/160 s |  | 5 = 1/125 s 6 = 1/100 s 7 = 1/80 s 8 = 1/60 s
> 15.2 | FlashShutterSpeed | int8u | [val & 0xf]
> 0 = 1/60 s 1 = 1/30 s 2 = 1/15 s 3 = 1/8 s 4 = 1/4 s 5 = 1/2 s |  | 6 = 1 s 7 = 2 s 8 = 4 s 9 = 8 s 10 = 15 s 11 = 30 s
> 16.1 | FlashControlBuilt-in | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Manual 2 = Repeating Flash 3 = Commander Mode
> 16.2 | ManualFlashOutput | int8u | [val & 0x1f]
> 17.1 | RepeatingFlashOutput | int8u | [val >> 4 & 0x7]
> 17.2 | RepeatingFlashCount | int8u | [val & 0xf]
> 18.1 | RepeatingFlashRate | int8u | [val >> 4 & 0xf]
> 18.2 | CommanderInternalTTLChannel | int8u | [val & 0x3] 0 = 1 ch 1 = 2 ch 2 = 3 ch 3 = 4 ch
> 20.1 | CommanderInternalTTLCompBuiltin | int8u | [val & 0x1f]
> 21.1 | CommanderInternalTTLCompGroupA | int8u | [val & 0x1f]
> 22.1 | CommanderInternalTTLCompGroupB | int8u | [val & 0x1f]
> 26.1 | AutoBracketSet | int8u | [val >> 6 & 0x3] 0 = AE & Flash 1 = AE Only 2 = Flash Only 3 = WB Bracketing
> 26.2 | AutoBracketModeM | int8u | [val >> 4 & 0x3] 0 = Flash/Speed 1 = Flash/Speed/Aperture 2 = Flash/Aperture 3 = Flash Only
> 26.3 | AutoBracketOrder | int8u | [val >> 3 & 0x1] 0 = 0,-,+ 1 = -,0,+
> 26.4 | ModelingFlash | int8u | [val & 0x1] 0 = On 1 = Off
> 27.1 | MultiSelectorShootMode | int8u | [val >> 6 & 0x3] 0 = Select Center Focus Point 1 = Highlight Active Focus Point 2 = Not Used
> 27.2 | MultiSelectorPlaybackMode | int8u | [val >> 4 & 0x3] 0 = Thumbnail On/Off 1 = View Histograms 2 = Zoom On/Off 3 = Choose Folder
> 27.3 | InitialZoomSetting | int8u | [val >> 2 & 0x3] 0 = Low Magnification 1 = Medium Magnification 2 = High Magnification
> 27.4 | MultiSelector | int8u | [val & 0x1] 0 = Do Nothing 1 = Reset Meter-off Delay
> 28.1 | FuncButton | int8u | [val >> 3 & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 9 = Flash Off 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = My Menu Top 15 = Live View 16 = + NEF (RAW) 17 = Virtual Horizon
> 29.1 | PreviewButton | int8u | [val >> 3 & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-ON 9 = Flash Off 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = My Menu Top 15 = Live View 16 = + NEF (RAW) 17 = Virtual Horizon
> 30.1 | AELockButton | int8u | (D300) [val >> 3 & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-ON 9 = Flash Off 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = My Menu Top 15 = Live View 16 = + NEF (RAW) 17 = Virtual Horizon
> 31.1 | FuncButtonPlusDials | int8u | [val >> 4 & 0x7]
> 0 = None 1 = Choose Image Area 2 = One Step Speed/Aperture 3 = Choose Non-CPU Lens Number 5 = Auto bracketing 6 = Dynamic AF Area 7 = Shutter speed & Aperture lock
> 31.2 | PreviewButtonPlusDials | int8u | [val & 0x7]
> 0 = None 1 = Choose Image Area 2 = One Step Speed/Aperture 3 = Choose Non-CPU Lens Number 5 = Auto bracketing 6 = Dynamic AF Area 7 = Shutter speed & Aperture lock
> 32.1 | AELockButtonPlusDials | int8u | [val >> 4 & 0x7]
> 33.1 | CommandDialsReverseRotation | int8u | [val >> 7 & 0x1] 0 = No 1 = Yes
> 33.2 | CommandDialsChangeMainSub | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 33.3 | CommandDialsApertureSetting | int8u | [val >> 5 & 0x1] 0 = Sub-command Dial 1 = Aperture Ring
> 33.4 | CommandDialsMenuAndPlayback | int8u | [val >> 4 & 0x1] 0 = Off 1 = On
> 33.5 | ReverseIndicators | int8u | [val >> 3 & 0x1] 0 = + 0 - 1 = - 0 +
> 33.6 | PhotoInfoPlayback | int8u | [val >> 2 & 0x1] 0 = Off 1 = On
> 33.7 | NoMemoryCard | int8u | [val >> 1 & 0x1] 0 = Release Locked 1 = Enable Release
> 33.8 | ReleaseButtonToUseDial | int8u | [val & 0x1] 0 = No 1 = Yes

## NikonCustom SettingsD800 Tags

Custom settings for the D800 and D800E.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 12.1 | AutoBracketingSet | int8u | [val >> 5 & 0x7] 0 = AE & Flash 1 = AE Only 2 = Flash Only 3 = WB Bracketing 4 = Active D-Lighting
> 12.2 | AutoBracketOrder | int8u | [val >> 4 & 0x1] 0 = 0,-,+ 1 = -,0,+
> 12.3 | AutoBracketingMode | int8u | [val >> 2 & 0x3] 0 = Flash/Speed 1 = Flash/Speed/Aperture 2 = Flash/Aperture 3 = Flash Only
> 22.1 | FlashSyncSpeed | int8u | [val >> 4 & 0xf]
> 0 = 1/320 s (auto FP) 1 = 1/250 s (auto FP) 2 = 1/250 s 3 = 1/200 s 4 = 1/160 s |  | 5 = 1/125 s 6 = 1/100 s 7 = 1/80 s 8 = 1/60 s
> 22.2 | FlashShutterSpeed | int8u | [val & 0xf]
> 0 = 1/60 s 1 = 1/30 s 2 = 1/15 s 3 = 1/8 s 4 = 1/4 s 5 = 1/2 s |  | 6 = 1 s 7 = 2 s 8 = 4 s 9 = 8 s 10 = 15 s 11 = 30 s
> 23.1 | FlashControlBuilt-in | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Manual 2 = Repeating Flash 3 = Commander Mode
> 23.2 | ManualFlashOutput | int8u | [val & 0x1f]
> 24.1 | RepeatingFlashOutput | int8u | [val >> 4 & 0x7]
> 24.2 | RepeatingFlashCount | int8u | [val & 0xf]
> 25.1 | RepeatingFlashRate | int8u | [val >> 4 & 0xf]
> 25.2 | CommanderChannel | int8u | [val & 0x3]
> 27.1 | CommanderInternalFlash | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Manual 2 = Off
> 27.2 | CommanderInternalManualOutput | int8u | [val & 0x1f]
> 28.1 | CommanderGroupAMode | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Auto Aperture 2 = Manual 3 = Off
> 28.2 | CommanderGroupAManualOutput | int8u | [val & 0x1f]
> 29.1 | CommanderGroupBMode | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Auto Aperture 2 = Manual 3 = Off
> 29.2 | CommanderGroupBManualOutput | int8u | [val & 0x1f]
> 30.1 | ModelingFlash | int8u | [val >> 5 & 0x1] 0 = On 1 = Off
> 30.2 | CommanderInternalTTLComp | int8u | [val & 0x1f]
> 31.1 | CommanderGroupA_TTL-AAComp | int8u | [val & 0x1f]
> 32.1 | CommanderGroupB_TTL-AAComp | int8u | [val & 0x1f]

## NikonCustom SettingsD810 Tags

Custom settings for the D810.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | LightSwitch | int8u | [val >> 3 & 0x1] 0 = LCD Backlight 1 = LCD Backlight and Shooting Information
> 0.2 | CustomSettingsBank | int8u | [val & 0x3] 0 = A 1 = B 2 = C 3 = D
> 1.1 | AF-CPrioritySelection | int8u | [val >> 6 & 0x3] 0 = Release 1 = Release + Focus 2 = Focus
> 1.2 | AF-SPrioritySelection | int8u | [val >> 5 & 0x1] 0 = Focus 1 = Release
> 1.3 | AFPointSelection | int8u | [val >> 4 & 0x1] 0 = 51 Points 1 = 11 Points
> 1.4 | FocusTrackingLockOn | int8u | [val & 0x7]
> 0 = Off 1 = 1 (Short) 2 = 2 |  | 3 = 3 (Normal) 4 = 4 5 = 5 (Long)
> 2.1 | AFActivation | int8u | [val >> 7 & 0x1] 0 = Shutter/AF-On 1 = AF-On Only
> 2.2 | FocusPointWrap | int8u | [val >> 3 & 0x1] 0 = No Wrap 1 = Wrap
> 2.3 | AFPointBrightness | int8u | [val >> 1 & 0x3] 0 = Auto 1 = On 2 = Off
> 2.4 | AFAssist | int8u | [val & 0x1] 0 = On 1 = Off
> 3.1 | BatteryOrder | int8u | [val >> 6 & 0x1] 0 = MB-D12 First 1 = Camera Battery First
> 3.2 | MB-D12BatteryType | int8u | [val & 0x3] 0 = LR6 (AA alkaline) 1 = HR6 (AA Ni-MH) 2 = FR6 (AA lithium)
> 4.1 | Pitch | int8u | [val >> 6 & 0x1] 0 = High 1 = Low
> 4.2 | NoMemoryCard | int8u | [val >> 5 & 0x1] 0 = Release Locked 1 = Enable Release
> 4.3 | ISODisplay | int8u | [val >> 2 & 0x3] 0 = Show ISO/Easy ISO 1 = Show ISO Sensitivity 3 = Show Frame Count
> 4.4 | GridDisplay | int8u | [val >> 1 & 0x1] 0 = On 1 = Off
> 5.1 | ShootingInfoDisplay | int8u | [val >> 6 & 0x3] 0 = Not Set 1 = Auto 2 = Manual (dark on light) 3 = Manual (light on dark)
> 5.2 | LCDIllumination | int8u | [val >> 5 & 0x1] 0 = Off 1 = On
> 5.3 | ElectronicFront-CurtainShutter | int8u | [val >> 3 & 0x1] 0 = Off 1 = On
> 5.4 | ScreenTips | int8u | [val >> 2 & 0x1] 0 = Off 1 = On
> 5.5 | Beep | int8u | [val & 0x3] 0 = Off 1 = Low 2 = Medium 3 = High
> 6.1 | ReverseIndicators | int8u | [val >> 7 & 0x1] 0 = + 0 - 1 = - 0 +
> 6.2 | CommandDialsReverseRotation | int8u | [val >> 3 & 0x3] 0 = No 1 = Shutter Speed & Aperture 2 = Exposure Compensation 3 = Exposure Compensation, Shutter Speed & Aperture
> 6.3 | EasyExposureCompensation | int8u | [val & 0x3] 0 = Off 1 = On 2 = On (auto reset)
> 7.1 | ExposureControlStepSize | int8u | [val >> 6 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 7.2 | ISOStepSize | int8u | [val >> 4 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 7.3 | ExposureCompStepSize | int8u | [val >> 2 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 8.1 | CenterWeightedAreaSize | int8u | [val >> 5 & 0x7] 0 = 8 mm 1 = 12 mm 2 = 15 mm 3 = 20 mm 4 = Average
> 8.2 | FineTuneOptMatrixMetering | int8u | [val & 0xf]
> 9.1 | FineTuneOptCenterWeighted | int8u | [val >> 4 & 0xf]
> 9.2 | FineTuneOptSpotMetering | int8u | [val & 0xf]
> 10.1 | MultiSelectorShootMode | int8u | [val >> 6 & 0x3] 0 = Select Center Focus Point (Reset) 1 = Highlight Active Focus Point 2 = Preset Focus Point (Pre) 3 = Not Used (None)
> 10.2 | MultiSelectorPlaybackMode | int8u | [val >> 4 & 0x3] 0 = Thumbnail On/Off 1 = View Histograms 2 = Zoom On/Off 3 = Choose Folder
> 10.3 | MultiSelector | int8u | [val & 0x1] 0 = Do Nothing 1 = Reset Meter-off Delay
> 11.1 | ExposureDelayMode | int8u | [val >> 6 & 0x3] 0 = Off 1 = 1 s 2 = 2 s 3 = 3 s
> 11.2 | CLModeShootingSpeed | int8u | [val & 0xf]
> 12.1 | MaxContinuousRelease | int8u |
> 13.1 | AutoBracketSet | int8u | [val >> 5 & 0x7] 0 = AE & Flash 1 = AE Only 2 = Flash Only 3 = WB Bracketing 4 = Active D-Lighting
> 13.2 | AutoBracketOrder | int8u | [val >> 4 & 0x1] 0 = 0,-,+ 1 = -,0,+
> 13.3 | AutoBracketModeM | int8u | [val >> 2 & 0x3] 0 = Flash/Speed 1 = Flash/Speed/Aperture 2 = Flash/Aperture 3 = Flash Only
> 14.1 | FuncButton | int8u | [val & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 19 = Grid Display 20 = My Menu 21 = Disable Synchronized Release 22 = Remote Release Only 26 = Flash Disable/Enable 27 = Highlight-weighted Metering
> 15.1 | PreviewButton | int8u | [val & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 19 = Grid Display 20 = My Menu 21 = Disable Synchronized Release 22 = Remote Release Only 26 = Flash Disable/Enable 27 = Highlight-weighted Metering
> 16.1 | AssignBktButton | int8u | [val & 0x7] 0 = Auto Bracketing 1 = Multiple Exposure 2 = HDR (high dynamic range) 3 = None
> 17.1 | AELockButton | int8u | [val & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 19 = Grid Display 20 = My Menu 21 = Disable Synchronized Release 22 = Remote Release Only 26 = Flash Disable/Enable 27 = Highlight-weighted Metering
> 18.1 | CommandDialsChangeMainSub | int8u | [val >> 5 & 0x7]
> 0 = Autofocus Off, Exposure Off 1 = Autofocus Off, Exposure On 2 = Autofocus Off, Exposure On (Mode A) 4 = Autofocus On, Exposure Off 5 = Autofocus On, Exposure On 6 = Autofocus On, Exposure On (Mode A)
> 18.2 | CommandDialsMenuAndPlayback | int8u | [val >> 3 & 0x3] 0 = On 1 = Off 2 = On (Image Review Excluded)
> 18.3 | CommandDialsApertureSetting | int8u | [val >> 2 & 0x1] 0 = Sub-command Dial 1 = Aperture Ring
> 18.4 | ShutterReleaseButtonAE-L | int8u | [val >> 1 & 0x1] 0 = Off 1 = On
> 18.5 | ReleaseButtonToUseDial | int8u | [val & 0x1] 0 = No 1 = Yes
> 19.1 | StandbyTimer | int8u | [val >> 4 & 0xf]
> 0 = 4 s 1 = 6 s 3 = 10 s |  | 5 = 30 s 6 = 1 min 7 = 5 min |  | 8 = 10 min 9 = 30 min 10 = No Limit
> 20.1 | SelfTimerTime | int8u | [val >> 6 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 20.2 | SelfTimerShotInterval | int8u | [val >> 4 & 0x3] 0 = 0.5 s 1 = 1 s 2 = 2 s 3 = 3 s
> 20.3 | SelfTimerShotCount | int8u | [val & 0xf]
> 21.1 | ImageReviewMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 2 s 1 = 4 s 3 = 10 s 4 = 20 s |  | 5 = 1 min 6 = 5 min 7 = 10 min
> 21.2 | LiveViewMonitorOffTime | int8u | [val >> 2 & 0x7]
> 1 = 5 min 2 = 10 min 3 = 15 min |  | 4 = 20 min 5 = 30 min 6 = No Limit
> 22.1 | MenuMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 2 = 10 s 4 = 20 s |  | 5 = 1 min 6 = 5 min 7 = 10 min
> 22.2 | ShootingInfoMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 2 = 10 s 4 = 20 s |  | 5 = 1 min 6 = 5 min 7 = 10 min
> 23.1 | FlashSyncSpeed | int8u | [val >> 4 & 0xf]
> 0 = 1/320 s (auto FP) 2 = 1/250 s (auto FP) 3 = 1/250 s 5 = 1/200 s 6 = 1/160 s |  | 7 = 1/125 s 8 = 1/100 s 9 = 1/80 s 10 = 1/60 s
> 23.2 | FlashShutterSpeed | int8u | [val & 0xf]
> 0 = 1/60 s 1 = 1/30 s 2 = 1/15 s 3 = 1/8 s 4 = 1/4 s 5 = 1/2 s |  | 6 = 1 s 7 = 2 s 8 = 4 s 9 = 8 s 10 = 15 s 11 = 30 s
> 24.1 | FlashControlBuilt-in | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Manual 2 = Repeating Flash 3 = Commander Mode
> 31.1 | ModelingFlash | int8u | [val >> 5 & 0x1] 0 = On 1 = Off
> 36.1 | PlaybackMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 37.1 | MultiSelectorLiveView | int8u | [val >> 6 & 0x3] 0 = Reset 1 = Zoom 3 = Not Used
> 38.1 | ShutterSpeedLock | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 38.2 | ApertureLock | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 38.3 | MovieShutterButton | int8u | [val >> 5 & 0x1] 0 = Take Photo 1 = Record Movies
> 38.4 | FlashExposureCompArea | int8u | [val >> 2 & 0x1] 0 = Entire frame 1 = Background only
> 40.1 | MovieAELockButtonAssignment | int8u | [val & 0xf]
> 0 = None 3 = Index Marking 4 = View Photo Shooting Info 5 = AE/AF Lock 6 = AE Lock Only 7 = AE Lock (hold) 8 = AF Lock Only
> 41.1 | MovieFunctionButton | int8u | [val >> 4 & 0x7] 0 = None 1 = Power Aperture (open) 3 = Index Marking 4 = View Photo Shooting Info
> 41.2 | MoviePreviewButton | int8u | [val & 0x7] 0 = None 2 = Power Aperture (open) 3 = Index Marking 4 = View Photo Shooting Info
> 42.1 | FuncButtonPlusDials | int8u | [val & 0xf]
> 0 = None 1 = Choose Image Area (FX/DX/5:4) 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 8 = Exposure Delay Mode
> 43.1 | PreviewButtonPlusDials | int8u | [val & 0xf]
> 0 = None 1 = Choose Image Area (FX/DX/5:4) 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 8 = Exposure Delay Mode
> 44.1 | AELockButtonPlusDials | int8u | [val & 0xf] 0 = None 1 = Choose Image Area (FX/DX/5:4) 2 = Shutter Speed & Aperture Lock 4 = Choose Non-CPU Lens Number 8 = Exposure Delay Mode
> 45.1 | AssignMovieRecordButton | int8u | [val & 0xf] 0 = None 1 = Choose Image Area (FX/DX/5:4) 2 = Shutter Speed & Aperture Lock 9 = White Balance 10 = ISO Sensitivity
> 46.1 | FineTuneOptHighlightWeighted | int8u | [val & 0xf]
> 47.1 | DynamicAreaAFDisplay | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 47.2 | AFPointIllumination | int8u | [val >> 6 & 0x1] 0 = Off 1 = On During Manual Focusing
> 47.3 | StoreByOrientation | int8u | [val >> 3 & 0x3] 0 = Off 1 = Focus Point 2 = Focus Point and AF-area mode
> 47.4 | GroupAreaAFIllumination | int8u | [val >> 2 & 0x1] 0 = Squares 1 = Dots
> 48.1 | MatrixMetering | int8u | [val >> 7 & 0x1] 0 = Face Detection On 1 = Face Detection Off
> 48.2 | LiveViewButtonOptions | int8u | [val >> 4 & 0x3] 0 = Enable 2 = Disable
> 48.3 | AFModeRestrictions | int8u | [val & 0x3] 0 = No Restrictions 1 = AF-C 2 = AF-S
> 49.1 | LimitAFAreaModeSelection | int8u | [val >> 1 & 0x3f]
> 0x0 = No Restrictions Bit 0 = Auto-area Bit 1 = Group-area Bit 2 = 3D-tracking Bit 3 = Dynamic area (51 points) Bit 4 = Dynamic area (21 points) Bit 5 = Dynamic area (9 points)
> 50.1 | AF-OnForMB-D12 | int8u | [val & 0x7]
> 0 = AE/AF Lock 1 = AE Lock Only 2 = AF Lock Only 3 = AE Lock (hold) |  | 4 = AE Lock (reset) 5 = AF-On 6 = FV Lock 7 = Same As Fn Button
> 51.1 | AssignRemoteFnButton | int8u | [val & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 7 = AF Lock Only 8 = AF-On 16 = +NEF(RAW) 25 = Live View 26 = Flash Disable/Enable
> 52.1 | LensFocusFunctionButtons | int8u | [val & 0x3f]
> 3 = AE/AF Lock 4 = AE Lock Only 7 = AF Lock Only 21 = Disable Synchronized Release 22 = Remote Release Only 24 = Preset focus Point 26 = Flash Disable/Enable 32 = AF-Area Mode: Single-point AF 33 = AF-Area Mode: Dynamic-area AF (9 points) 34 = AF-Area Mode: Dynamic-area AF (21 points) 35 = AF-Area Mode: Dynamic-area AF (51 points) 36 = AF-Area Mode: Group-area AF 37 = AF-Area Mode: Auto area AF

## NikonCustom SettingsD850 Tags

Custom settings for the D850.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.2 | CustomSettingsBank | int8u | [val & 0x3] 0 = A 1 = B 2 = C 3 = D
> 1.1 | AF-CPrioritySelection | int8u | [val >> 6 & 0x3] 0 = Release 1 = Release + Focus 2 = Focus 3 = Focus + Release
> 1.2 | AF-SPrioritySelection | int8u | [val >> 5 & 0x1] 0 = Focus 1 = Release
> 1.3 | AFPointSelection | int8u | [val >> 4 & 0x1] 0 = 55 Points 1 = 15 Points
> 1.4 | Three-DTrackingFaceDetection | int8u | [val >> 3 & 0x1] 0 = Off 1 = On
> 1.5 | BlockShotAFResponse | int8u | [val & 0x7] 1 = 1 (Quick) 2 = 2 3 = 3 (Normal) 4 = 4 5 = 5 (Delay)
> 2.1 | FocusPointWrap | int8u | [val >> 3 & 0x1] 0 = No Wrap 1 = Wrap
> 2.2 | AFPointBrightness | int8u | [val >> 1 & 0x3] 0 = Auto 1 = On 2 = Off
> 4.1 | ISODisplay | int8u | [val >> 3 & 0x1] 0 = Show ISO Sensitivity 1 = Show Frame Count
> 4.2 | GridDisplay | int8u | [val >> 1 & 0x1] 0 = On 1 = Off
> 5.1 | LCDIllumination | int8u | [val >> 5 & 0x1] 0 = Off 1 = On
> 5.2 | ElectronicFront-CurtainShutter | int8u | [val >> 3 & 0x1] 0 = Off 1 = On
> 6.1 | ReverseIndicators | int8u | [val >> 7 & 0x1] 0 = + 0 - 1 = - 0 +
> 6.2 | CommandDialsReverseRotation | int8u | [val >> 3 & 0x3] 0 = No 1 = Shutter Speed & Aperture 2 = Exposure Compensation 3 = Exposure Compensation, Shutter Speed & Aperture
> 6.3 | EasyExposureCompensation | int8u | [val & 0x3] 0 = Off 1 = On 2 = On (Auto Reset)
> 7.1 | ExposureControlStepSize | int8u | [val >> 6 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 7.2 | ISOStepSize | int8u | [val >> 4 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 7.3 | ExposureCompStepSize | int8u | [val >> 2 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 8.1 | CenterWeightedAreaSize | int8u | [val >> 5 & 0x7] 0 = 8 mm 1 = 12 mm 2 = 15 mm 3 = 20 mm 4 = Average
> 8.2 | FineTuneOptMatrixMetering | int8u | [val & 0xf]
> 9.1 | FineTuneOptCenterWeighted | int8u | [val >> 4 & 0xf]
> 9.2 | FineTuneOptSpotMetering | int8u | [val & 0xf]
> 10.1 | MultiSelectorShootMode | int8u | [val >> 5 & 0x7] 0 = Select Center Focus Point (Reset) 2 = Preset Focus Point (Pre) 3 = Highlight Active Focus Point 4 = Not Used (None)
> 10.2 | MultiSelectorPlaybackMode | int8u | [val >> 2 & 0x3] 0 = Thumbnail On/Off 1 = View Histograms 2 = Zoom On/Off 3 = Choose Folder
> 10.3 | MultiSelector | int8u | [val & 0x1] 0 = Do Nothing 1 = Reset Meter-off Delay
> 11.1 | ExposureDelayMode | int8u | [val >> 5 & 0x7]
> 0 = Off 1 = 0.2 s 2 = 0.5 s |  | 3 = 1 s 4 = 2 s 5 = 3 s
> 11.2 | CLModeShootingSpeed | int8u | [val & 0xf]
> 12.1 | MaxContinuousRelease | int8u |
> 13.1 | AutoBracketOrder | int8u | [val >> 4 & 0x1] 0 = 0,-,+ 1 = -,0,+
> 13.2 | AutoBracketModeM | int8u | [val >> 2 & 0x3] 0 = Flash/Speed 1 = Flash/Speed/Aperture 2 = Flash/Aperture 3 = Flash Only
> 14.1 | Func1Button | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 19 = Grid Display 20 = My Menu 22 = Remote Release Only 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 153 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 153 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only) 56 = AF-Area Mode (Dynamic Area 9 Points) 57 = AF-Area Mode + AF-On (Dynamic Area 9 Points)
> 15.1 | PreviewButton | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 19 = Grid Display 20 = My Menu 22 = Remote Release Only 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 153 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 153 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only) 56 = AF-Area Mode (Dynamic Area 9 Points) 57 = AF-Area Mode + AF-On (Dynamic Area 9 Points)
> 16.1 | AssignBktButton | int8u | [val & 0x7] 0 = Auto Bracketing 1 = Multiple Exposure 2 = HDR (high dynamic range) 3 = None
> 18.1 | CommandDialsChangeMainSub | int8u | [val >> 5 & 0x7]
> 0 = Autofocus Off, Exposure Off 1 = Autofocus Off, Exposure On 2 = Autofocus Off, Exposure On (Mode A) 4 = Autofocus On, Exposure Off 5 = Autofocus On, Exposure On 6 = Autofocus On, Exposure On (Mode A)
> 18.2 | CommandDialsMenuAndPlayback | int8u | [val >> 3 & 0x3] 0 = On 1 = Off 2 = On (Image Review Excluded)
> 18.3 | CommandDialsApertureSetting | int8u | [val >> 2 & 0x1] 0 = Sub-command Dial 1 = Aperture Ring
> 18.4 | ReleaseButtonToUseDial | int8u | [val & 0x1] 0 = No 1 = Yes
> 19.1 | StandbyTimer | int8u | [val >> 4 & 0xf]
> 0 = 4 s 1 = 6 s 3 = 10 s |  | 5 = 30 s 6 = 1 min 7 = 5 min |  | 8 = 10 min 9 = 30 min 10 = No Limit
> 20.1 | SelfTimerTime | int8u | [val >> 6 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 20.2 | SelfTimerShotInterval | int8u | [val >> 4 & 0x3] 0 = 0.5 s 1 = 1 s 2 = 2 s 3 = 3 s
> 20.3 | SelfTimerShotCount | int8u | [val & 0xf]
> 21.1 | ImageReviewMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 2 s 1 = 4 s 3 = 10 s 4 = 20 s |  | 5 = 1 min 6 = 5 min 7 = 10 min
> 21.2 | LiveViewMonitorOffTime | int8u | [val >> 2 & 0x7]
> 1 = 5 min 2 = 10 min 3 = 15 min |  | 4 = 20 min 5 = 30 min 6 = No Limit
> 22.1 | MenuMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 2 = 10 s 4 = 20 s |  | 5 = 1 min 6 = 5 min 7 = 10 min
> 22.2 | ShootingInfoMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 2 = 10 s 4 = 20 s |  | 5 = 1 min 6 = 5 min 7 = 10 min
> 23.1 | FlashSyncSpeed | int8u | [val >> 4 & 0xf]
> 2 = 1/250 s (auto FP) 3 = 1/250 s 5 = 1/200 s 6 = 1/160 s |  | 7 = 1/125 s 8 = 1/100 s 9 = 1/80 s 10 = 1/60 s
> 23.2 | FlashShutterSpeed | int8u | [val & 0xf]
> 0 = 1/60 s 1 = 1/30 s 2 = 1/15 s 3 = 1/8 s 4 = 1/4 s 5 = 1/2 s |  | 6 = 1 s 7 = 2 s 8 = 4 s 9 = 8 s 10 = 15 s 11 = 30 s
> 31.1 | ModelingFlash | int8u | [val >> 5 & 0x1] 0 = On 1 = Off
> 36.1 | PlaybackMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 37.1 | MultiSelectorLiveView | int8u | [val >> 6 & 0x3] 0 = Reset 1 = Zoom 3 = Not Used
> 38.1 | ShutterSpeedLock | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 38.2 | ApertureLock | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 38.3 | MovieShutterButton | int8u | [val >> 4 & 0x1] 0 = Take Photo 1 = Record Movies
> 38.4 | FlashExposureCompArea | int8u | [val >> 2 & 0x1] 0 = Entire Frame 1 = Background Only
> 38.5 | AutoFlashISOSensitivity | int8u | [val >> 1 & 0x1] 0 = Subject and Background 1 = Subject Only
> 41.1 | MovieFunc1Button | int8u | [val >> 4 & 0xf] 0 = None 2 = Power Aperture (close) 3 = Index Marking 4 = View Photo Shooting Info 11 = Exposure Compensation -
> 41.2 | MoviePreviewButton | int8u | [val & 0xf] 0 = None 1 = Power Aperture (open) 3 = Index Marking 4 = View Photo Shooting Info 10 = Exposure Compensation +
> 42.1 | Func1ButtonPlusDials | int8u | [val & 0xf]
> 0 = None 1 = Choose Image Area 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 7 = Photo Shooting Menu Bank 8 = Exposure Delay Mode
> 43.1 | PreviewButtonPlusDials | int8u | [val & 0xf]
> 0 = None 1 = Choose Image Area 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 7 = Photo Shooting Menu Bank 8 = Exposure Delay Mode
> 45.1 | AssignMovieRecordButtonPlusDials | int8u | [val & 0xf] 0 = None 1 = Choose Image Area 2 = Shutter Speed & Aperture Lock 7 = Photo Shooting Menu Bank 11 = Exposure Mode
> 46.1 | FineTuneOptHighlightWeighted | int8u | [val & 0xf]
> 47.1 | DynamicAreaAFDisplay | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 47.2 | AFPointIllumination | int8u | [val >> 6 & 0x1] 0 = Off 1 = On During Manual Focusing
> 47.3 | StoreByOrientation | int8u | [val >> 3 & 0x3] 0 = Off 1 = Focus Point 2 = Focus Point and AF-area Mode
> 48.1 | MatrixMetering | int8u | [val >> 7 & 0x1] 0 = Face Detection On 1 = Face Detection Off
> 48.2 | LiveViewButtonOptions | int8u | [val >> 4 & 0x3] 0 = Enable 1 = Enable (Standby Timer Active) 2 = Disable
> 48.3 | AFModeRestrictions | int8u | [val & 0x3] 0 = No Restrictions 1 = AF-C 2 = AF-S
> 49.1 | LimitAFAreaModeSelection | int8u | [val >> 1 & 0x3f]
> 0x0 = No Restrictions Bit 0 = Auto-area Bit 1 = Group-area Bit 2 = 3D-tracking Bit 3 = Dynamic area (153 points) Bit 4 = Dynamic area (72 points) Bit 5 = Dynamic area (25 points)
> 52.1 | LensFocusFunctionButtons | int8u | [val & 0x3f] 3 = AE/AF Lock 4 = AE Lock Only 7 = AF Lock Only 8 = AF-On 24 = Preset Focus Point 26 = Flash Disable/Enable 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 153 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 153 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only) 56 = AF-Area Mode (Dynamic Area 9 Points) 57 = AF-Area Mode + AF-On (Dynamic Area 9 Points)
> 66.1 | VerticalMultiSelector | int8u | [val & 0xff] 0x0 = Same as Multi-Selector with Info(U/D) & Playback(R/L) 0x8 = Same as Multi-Selector with Info(R/L) & Playback(U/D) 0x80 = Focus Point Selection
> 67.1 | AssignMB-D18FuncButton | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 18 = Reset Focus Point 19 = Grid Display 20 = My Menu 22 = Remote Release Only 23 = Preset Focus Point 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 153 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 153 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only) 54 = Highlight Active Focus Point 56 = AF-Area Mode (Dynamic Area 9 Points) 57 = AF-Area Mode + AF-On (Dynamic Area 9 Points)
> 68.1 | AssignMB-D18FuncButtonPlusDials | int8u | [val & 0xf]
> 0 = None 1 = Choose Image Area 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 7 = Photo Shooting Menu Bank 8 = Exposure Delay Mode 10 = ISO Sensitivity 11 = Exposure Mode 12 = Exposure Compensation 13 = Metering Mode
> 70.1 | AF-OnButton | int8u | [val & 0x3f] 0 = None 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 153 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 153 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 56 = AF-Area Mode (Dynamic Area 9 Points) 57 = AF-Area Mode + AF-On (Dynamic Area 9 Points)
> 71.1 | SubSelector | int8u | [val >> 7 & 0x1] 0 = Focus Point Selection 1 = Same as MultiSelector
> 72.1 | SubSelectorCenter | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 18 = Reset Focus Point 19 = Grid Display 20 = My Menu 22 = Remote Release Only 23 = Preset Focus Point 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 153 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 153 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only) 54 = Highlight Active Focus Point 56 = AF-Area Mode (Dynamic Area 9 Points) 57 = AF-Area Mode + AF-On (Dynamic Area 9 Points)
> 73.1 | SubSelectorPlusDials | int8u | [val & 0xf] 0 = None 1 = Choose Image Area 2 = Shutter Speed & Aperture Lock 4 = Choose Non-CPU Lens Number 7 = Photo Shooting Menu Bank
> 74.1 | AssignMovieSubselector | int8u | [val >> 4 & 0xf]
> 0 = None 3 = Index Marking 4 = View Photo Shooting Info 5 = AE/AF Lock 6 = AE Lock (Only) 7 = AE Lock (Hold) 8 = AF Lock (Only)
> 75.1 | AssignMovieFunc1ButtonPlusDials | int8u | [val >> 4 & 0x1] 0 = None 1 = Choose Image Area
> 75.2 | AssignMoviePreviewButtonPlusDials | int8u | [val & 0x1] 0 = None 1 = Choose Image Area
> 76.1 | AssignMovieSubselectorPlusDials | int8u | [val >> 4 & 0x1] 0 = None 1 = Choose Image Area
> 77.1 | SyncReleaseMode | int8u | [val >> 7 & 0x1] 0 = No Sync 1 = Sync
> 77.2 | ContinuousModeLiveView | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 78.1 | Three-DTrackingWatchArea | int8u | [val >> 7 & 0x1] 0 = Wide 1 = Normal
> 78.2 | SubjectMotion | int8u | [val >> 5 & 0x3] 0 = Steady 1 = Middle 2 = Erratic
> 78.3 | AFActivation | int8u | [val >> 3 & 0x1] 0 = Shutter/AF-On 1 = AF-On Only
> 78.4 | ShutterReleaseButtonAE-L | int8u | [val & 0x3] 0 = Off 1 = On (Half Press) 2 = On (Burst Mode)
> 79.1 | AssignMB-D18AF-OnButton | int8u | [val & 0x7f] 0 = None 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 153 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 153 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 56 = AF-Area Mode (Dynamic Area 9 Points) 57 = AF-Area Mode + AF-On (Dynamic Area 9 Points) 100 = Same as Camera AF-On Button
> 80.1 | Func2Button | int8u | [val & 0x3f] 0 = None 15 = My Menu Top Item 20 = My Menu 55 = Rating
> 82.1 | AssignMovieFunc2Button | int8u | [val >> 4 & 0x7] 0 = None 3 = Index Marking 4 = View Photo Shooting Info

## NikonCustom SettingsD5000 Tags

Custom settings for the D5000.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | AFAreaModeSetting | int8u | [val >> 5 & 0x3] 0 = Single Area 1 = Dynamic Area 2 = Auto-area 3 = 3D-tracking (11 points)
> 0.2 | AFAssist | int8u | [val & 0x1] 0 = On 1 = Off
> 2.1 | Beep | int8u | [val >> 6 & 0x3] 0 = Off 1 = Low 2 = High
> 2.2 | GridDisplay | int8u | [val >> 1 & 0x1] 0 = On 1 = Off
> 2.3 | ISODisplay | int8u | [val >> 3 & 0x1] 0 = On 1 = Off
> 2.4 | NoMemoryCard | int8u | [val >> 5 & 0x1] 0 = Release Locked 1 = Enable Release
> 3.1 | FileNumberSequence | int8u | [val >> 3 & 0x1] 0 = On 1 = Off
> 4.1 | RangeFinder | int8u | [val >> 4 & 0x1] 0 = Off 1 = On
> 4.2 | DateImprint | int8u | [val >> 3 & 0x1] 0 = Off 1 = On
> 4.3 | ReverseIndicators | int8u | [val >> 7 & 0x1] 0 = + 0 - 1 = - 0 +
> 5.1 | EVStepSize | int8u | [val >> 6 & 0x1] 0 = 1/3 EV 1 = 1/2 EV
> 9.1 | ExposureDelayMode | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 11.1 | AutoBracketSet | int8u | [val >> 6 & 0x3] 0 = Exposure 1 = Active D-Lighting 2 = WB Bracketing
> 12.1 | TimerFunctionButton | int8u | [val >> 3 & 0x7]
> 0 = Self-timer 1 = Release Mode 2 = Image Quality/Size 3 = ISO |  | 4 = White Balance 5 = Active D-Lighting 6 = + NEF (RAW) 7 = Auto Bracketing
> 15.1 | AELockButton | int8u | [val >> 3 & 0x7] 0 = AE/AF Lock 1 = AE Lock Only 2 = AF Lock Only 3 = AE Lock (hold) 4 = AF-ON
> 16.1 | ShutterReleaseButtonAE-L | int8u | [val >> 1 & 0x1] 0 = Off 1 = On
> 16.2 | CommandDialsReverseRotation | int8u | [val >> 7 & 0x1] 0 = No 1 = Yes
> 17.1 | MeteringTime | int8u | [val >> 4 & 0x7] 0 = 4 s 1 = 8 s 2 = 20 s 3 = 1 min 4 = 30 min
> 17.2 | RemoteOnDuration | int8u | [val & 0x3] 0 = 1 min 1 = 5 min 2 = 10 min 3 = 15 min
> 18.1 | SelfTimerTime | int8u | [val >> 6 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 18.2 | SelfTimerShotCount | int8u | [val >> 1 & 0xf]
> 19.1 | ImageReviewTime | int8u | [val >> 5 & 0x7] 0 = 4 s 1 = 8 s 2 = 20 s 3 = 1 min 4 = 10 min
> 20.1 | PlaybackMenusTime | int8u | [val >> 5 & 0x7] 0 = 8 s 1 = 12 s 2 = 20 s 3 = 1 min 4 = 10 min
> 22.1 | InternalFlash | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Manual
> 22.2 | ManualFlashOutput | int8u | [val & 0x1f]
> 32.1 | LiveViewAF | int8u | [val >> 5 & 0x3] 0 = Face Priority 1 = Wide Area 2 = Normal Area 3 = Subject Tracking

## NikonCustom SettingsD5100 Tags

Custom settings for the D5100.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | AF-CPrioritySelection | int8u | [val >> 7 & 0x1] 0 = Release 1 = Focus
> 1.1 | AFAssist | int8u | [val & 0x1] 0 = On 1 = Off
> 3.1 | Beep | int8u | [val >> 6 & 0x3] 0 = Off 1 = Low 2 = High
> 3.2 | NoMemoryCard | int8u | [val >> 5 & 0x1] 0 = Release Locked 1 = Enable Release
> 3.3 | ISODisplay | int8u | [val >> 3 & 0x1] 0 = On 1 = Off
> 4.1 | FileNumberSequence | int8u | [val >> 3 & 0x1] 0 = On 1 = Off
> 5.1 | RangeFinder | int8u | [val >> 4 & 0x1] 0 = Off 1 = On
> 5.2 | ReverseIndicators | int8u | [val >> 7 & 0x1] 0 = + 0 - 1 = - 0 +
> 6.1 | EVStepSize | int8u | [val >> 6 & 0x1] 0 = 1/3 EV 1 = 1/2 EV
> 10.1 | ExposureDelayMode | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 12.1 | AutoBracketSet | int8u | [val >> 6 & 0x3] 0 = Exposure 1 = WB Bracketing 2 = Active D-Lighting
> 13.1 | TimerFunctionButton | int8u | [val >> 3 & 0x7]
> 0 = Self-timer 1 = Release Mode 2 = Image Quality/Size 3 = ISO |  | 4 = White Balance 5 = Active D-Lighting 6 = + NEF (RAW) 7 = Auto Bracketing
> 16.1 | AELockButton | int8u | [val >> 3 & 0x7] 0 = AE/AF Lock 1 = AE Lock Only 2 = AF Lock Only 3 = AE Lock (hold) 4 = AF-ON
> 17.1 | ShutterReleaseButtonAE-L | int8u | [val >> 1 & 0x1] 0 = Off 1 = On
> 17.2 | CommandDialsReverseRotation | int8u | [val >> 7 & 0x1] 0 = No 1 = Yes
> 18.1 | MeteringTime | int8u | [val >> 4 & 0x7] 0 = 4 s 1 = 8 s 2 = 20 s 3 = 1 min 4 = 30 min
> 18.2 | RemoteOnDuration | int8u | [val & 0x3] 0 = 1 min 1 = 5 min 2 = 10 min 3 = 20 min
> 19.1 | SelfTimerTime | int8u | [val >> 6 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 19.2 | SelfTimerShotCount | int8u | [val & 0xf]
> 20.1 | ImageReviewTime | int8u | [val >> 5 & 0x7] 0 = 4 s 1 = 8 s 2 = 20 s 3 = 1 min 4 = 10 min
> 20.2 | LiveViewMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 3 min 1 = 5 min 2 = 10 min |  | 3 = 15 min 4 = 20 min 5 = 30 min
> 21.1 | PlaybackMenusTime | int8u | [val >> 5 & 0x7] 0 = 8 s 1 = 12 s 2 = 20 s 3 = 1 min 4 = 10 min
> 23.1 | ManualFlashOutput | int8u | [val & 0x1f]

## NikonCustom SettingsD5200 Tags

Custom settings for the D5200.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | AF-CPrioritySelection | int8u | [val >> 7 & 0x1] 0 = Release 1 = Focus
> 0.2 | NumberOfFocusPoints | int8u | [val >> 4 & 0x1] 0 = 39 Points 1 = 11 Points
> 1.1 | AFAssist | int8u | [val & 0x1] 0 = On 1 = Off
> 3.1 | Beep | int8u | [val >> 6 & 0x3] 0 = Off 1 = Low 2 = High
> 3.2 | NoMemoryCard | int8u | [val >> 5 & 0x1] 0 = Release Locked 1 = Enable Release
> 3.3 | ISODisplay | int8u | [val >> 3 & 0x1] 0 = On 1 = Off
> 4.1 | FileNumberSequence | int8u | [val >> 3 & 0x1] 0 = On 1 = Off
> 5.1 | RangeFinder | int8u | [val >> 2 & 0x1] 0 = Off 1 = On
> 5.2 | ReverseExposureCompDial | int8u | [val >> 4 & 0x1] 0 = No 1 = Yes
> 5.3 | ReverseShutterSpeedAperture | int8u | [val >> 3 & 0x1] 0 = No 1 = Yes
> 5.4 | ReverseIndicators | int8u | [val >> 7 & 0x1] 0 = + 0 - 1 = - 0 +
> 6.1 | EVStepSize | int8u | [val >> 6 & 0x1] 0 = 1/3 EV 1 = 1/2 EV
> 10.1 | ExposureDelayMode | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 12.1 | AutoBracketSet | int8u | [val >> 6 & 0x3] 0 = Exposure 1 = WB Bracketing 2 = Active D-Lighting
> 13.1 | FunctionButton | int8u | [val & 0x1f]
> 3 = AE/AF Lock 4 = AE Lock Only 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-ON 16 = + NEF (RAW) 18 = Active D-Lighting |  | 25 = Live View 26 = Image Quality 27 = ISO 28 = White Balance 29 = HDR 30 = Auto Bracketing 31 = AF-area Mode
> 16.1 | AELockButton | int8u | [val & 0xf] 3 = AE/AF Lock 4 = AE Lock Only 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-ON
> 17.1 | ShutterReleaseButtonAE-L | int8u | [val >> 1 & 0x1] 0 = Off 1 = On
> 18.1 | StandbyTimer | int8u | [val >> 5 & 0x7] 0 = 4 s 1 = 8 s 2 = 20 s 3 = 1 min 4 = 30 min
> 18.2 | RemoteOnDuration | int8u | [val & 0x3] 0 = 1 min 1 = 5 min 2 = 10 min 3 = 15 min
> 19.1 | SelfTimerTime | int8u | [val >> 6 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 19.2 | SelfTimerShotCount | int8u | [val & 0xf]
> 20.1 | ImageReviewTime | int8u | [val >> 5 & 0x7] 1 = 4 s 2 = 8 s 4 = 20 s 5 = 1 min 7 = 10 min
> 20.2 | LiveViewMonitorOffTime | int8u | [val >> 2 & 0x7] 1 = 5 min 2 = 10 min 3 = 15 min 4 = 20 min 5 = 30 min
> 21.1 | PlaybackMenusTime | int8u | [val >> 5 & 0x7] 1 = 8 s 4 = 20 s 5 = 1 min 6 = 5 min 7 = 10 min
> 23.1 | InternalFlash | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Manual
> 23.2 | ManualFlashOutput | int8u | [val & 0x1f]

## NikonCustom SettingsD7000 Tags

Custom settings for the D7000.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | AF-CPrioritySelection | int8u | [val >> 7 & 0x1] 0 = Release 1 = Focus
> 0.2 | AF-SPrioritySelection | int8u | [val >> 5 & 0x1] 0 = Focus 1 = Release
> 0.3 | NumberOfFocusPoints | int8u | [val >> 4 & 0x1] 0 = 39 Points 1 = 11 Points
> 0.4 | FocusTrackingLockOn | int8u | [val & 0x7]
> 0 = Off 1 = 1 Short 2 = 2 |  | 3 = 3 Normal 4 = 4 5 = 5 Long
> 1.1 | FocusPointWrap | int8u | [val >> 3 & 0x1] 0 = No Wrap 1 = Wrap
> 1.2 | AFPointIllumination | int8u | [val >> 1 & 0x3] 0 = Auto 1 = On 2 = Off
> 1.3 | AFAssist | int8u | [val & 0x1] 0 = On 1 = Off
> 2.1 | BatteryOrder | int8u | [val >> 6 & 0x1] 0 = MB-D11 First 1 = Camera Battery First
> 2.2 | AF-OnForMB-D11 | int8u | [val >> 2 & 0x7]
> 0 = AE/AF Lock 1 = AE Lock Only 2 = AF Lock Only 3 = AE Lock (hold) |  | 4 = AF-ON 5 = FV Lock 6 = Same as FUNC Button
> 2.3 | MB-D11BatteryType | int8u | [val & 0x3] 0 = LR6 (AA alkaline) 1 = Ni-MH (AA Ni-MH) 2 = FR6 (AA lithium)
> 3.1 | BeepPitch | int8u | [val >> 6 & 0x3] 0 = Off 1 = Low 2 = High
> 3.2 | NoMemoryCard | int8u | [val >> 5 & 0x1] 0 = Release Locked 1 = Enable Release
> 3.3 | ISODisplay | int8u | [val >> 2 & 0x3] 0 = Show ISO/Easy ISO 1 = Show ISO Sensitivity 3 = Show Frame Count
> 3.4 | GridDisplay | int8u | [val >> 1 & 0x1] 0 = On 1 = Off
> 3.5 | ViewfinderWarning | int8u | [val & 0x1] 0 = On 1 = Off
> 4.1 | ShootingInfoDisplay | int8u | [val >> 6 & 0x3] 0 = Auto 2 = Manual (dark on light) 3 = Manual (light on dark)
> 4.2 | LCDIllumination | int8u | [val >> 5 & 0x1] 0 = Off 1 = On
> 4.3 | FileNumberSequence | int8u | [val >> 3 & 0x1] 0 = On 1 = Off
> 4.4 | ScreenTips | int8u | [val >> 2 & 0x1] 0 = Off 1 = On
> 4.5 | BeepVolume | int8u | [val & 0x3] 0 = Off 1 = 1 2 = 2 3 = 3
> 5.1 | ReverseIndicators | int8u | [val >> 7 & 0x1] 0 = + 0 - 1 = - 0 +
> 5.2 | EasyExposureCompensation | int8u | [val & 0x3] 0 = Off 1 = On 2 = On Auto Reset
> 6.1 | ExposureControlStep | int8u | [val >> 6 & 0x1] 0 = 1/3 EV 1 = 1/2 EV
> 6.2 | ISOSensitivityStep | int8u | [val >> 4 & 0x1] 0 = 1/3 EV 1 = 1/2 EV
> 7.1 | CenterWeightedAreaSize | int8u | [val >> 5 & 0x7] 0 = 6 mm 1 = 8 mm 2 = 10 mm 3 = 13 mm 4 = Average
> 10.1 | ExposureDelayMode | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 10.2 | CLModeShootingSpeed | int8u | [val & 0x7]
> 11 | MaxContinuousRelease | int8u |
> 12.1 | AutoBracketSet | int8u | [val >> 5 & 0x7] 0 = AE & Flash 1 = AE Only 2 = Flash Only 3 = WB Bracketing 4 = Active D-Lighting
> 12.2 | AutoBracketOrder | int8u | [val >> 4 & 0x1] 0 = 0,-,+ 1 = -,0,+
> 13.1 | FuncButton | int8u | [val >> 3 & 0x1f]
> 0 = Grid Display 1 = FV Lock 2 = Flash Off 3 = Matrix Metering 4 = Center-weighted Metering 5 = Spot Metering 6 = My Menu Top 7 = + NEF (RAW) 8 = Active D-Lighting 9 = Preview 10 = AE/AF Lock 11 = AE Lock Only 12 = AF Lock Only 13 = AE Lock (hold) 14 = Bracketing Burst 15 = Playback 16 = 1EV Step Speed/Aperture 17 = Choose Non-CPU Lens 18 = Virtual Horizon 19 = Start Movie Recording
> 14.1 | PreviewButton | int8u | [val >> 3 & 0x1f]
> 0 = Grid Display 1 = FV Lock 2 = Flash Off 3 = Matrix Metering 4 = Center-weighted Metering 5 = Spot Metering 6 = My Menu Top 7 = + NEF (RAW) 8 = Active D-Lighting 9 = Preview 10 = AE/AF Lock 11 = AE Lock Only 12 = AF Lock Only 13 = AE Lock (hold) 14 = Bracketing Burst 15 = Playback 16 = 1EV Step Speed/Aperture 17 = Choose Non-CPU Lens 18 = Virtual Horizon 19 = Start Movie Recording
> 15.1 | OKButton | int8u | [val >> 3 & 0x3] 0 = Off 1 = Select Center Focus Point 2 = Highlight Active Focus Point 3 = Not Used
> 16.1 | AELockButton | int8u | [val >> 3 & 0x7]
> 0 = AE/AF Lock 1 = AE Lock Only 2 = AF Lock Only |  | 3 = AE Lock (hold) 4 = AF-ON 5 = FV Lock
> 17.1 | CommandDialsReverseRotation | int8u | [val >> 7 & 0x1] 0 = No 1 = Yes
> 17.2 | CommandDialsChangeMainSub | int8u | [val >> 5 & 0x3] 0 = Off 1 = On 2 = On (A mode only)
> 17.3 | CommandDialsApertureSetting | int8u | [val >> 2 & 0x1] 0 = Sub-command Dial 1 = Aperture Ring
> 17.4 | CommandDialsMenuAndPlayback | int8u | [val >> 3 & 0x3] 0 = On 1 = Off 2 = On (Image Review Exclude)
> 17.5 | ShutterReleaseButtonAE-L | int8u | [val >> 1 & 0x1] 0 = Off 1 = On
> 17.6 | ReleaseButtonToUseDial | int8u | [val & 0x1] 0 = No 1 = Yes
> 18.1 | MeteringTime | int8u | [val >> 4 & 0xf]
> 0 = 4 s 1 = 6 s 2 = 8 s 3 = 16 s 4 = 30 s |  | 5 = 1 min 6 = 5 min 7 = 10 min 8 = 30 min 9 = No Limit
> 18.2 | RemoteOnDuration | int8u | [val & 0x3] 0 = 1 min 1 = 5 min 2 = 10 min 3 = 15 min
> 19.1 | SelfTimerTime | int8u | [val >> 6 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 19.2 | SelfTimerInterval | int8u | [val >> 4 & 0x3] 0 = 0.5 s 1 = 1 s 2 = 2 s 3 = 3 s
> 19.3 | SelfTimerShotCount | int8u | [val & 0xf]
> 20.1 | ImageReviewTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 20.2 | LiveViewMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 21.1 | MenuMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 21.2 | ShootingInfoMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 22.1 | FlashSyncSpeed | int8u | [val >> 4 & 0xf]
> 0 = 1/320 s (auto FP) 1 = 1/250 s (auto FP) 2 = 1/250 s 3 = 1/200 s 4 = 1/160 s |  | 5 = 1/125 s 6 = 1/100 s 7 = 1/80 s 8 = 1/60 s
> 22.2 | FlashShutterSpeed | int8u | [val & 0xf]
> 0 = 1/60 s 1 = 1/30 s 2 = 1/15 s 3 = 1/8 s 4 = 1/4 s 5 = 1/2 s |  | 6 = 1 s 7 = 2 s 8 = 4 s 9 = 8 s 10 = 15 s 11 = 30 s
> 23.1 | FlashControlBuilt-in | int8u | [val >> 6 & 0x3] 0 = TTL 1 = Manual 2 = Repeating Flash 3 = Commander Mode
> 23.2 | ManualFlashOutput | int8u | [val & 0x1f]
> 24.1 | RepeatingFlashOutput | int8u | [val >> 4 & 0x7]
> 24.2 | RepeatingFlashCount | int8u | [val & 0xf]
> 25.1 | RepeatingFlashRate | int8u | [val >> 4 & 0xf]
> 26.1 | CommanderInternalTTLCompBuiltin | int8u | [val & 0x1f]
> 27.1 | CommanderInternalTTLCompGroupA | int8u | [val & 0x1f]
> 28.1 | CommanderInternalTTLCompGroupB | int8u | [val & 0x1f]
> 30.1 | FlashWarning | int8u | [val >> 7 & 0x1] 0 = On 1 = Off
> 30.2 | ModelingFlash | int8u | [val >> 5 & 0x1] 0 = On 1 = Off
> 34.1 | LiveViewAFAreaMode | int8u | [val >> 5 & 0x3] 0 = Face-Priority 1 = NormalArea 2 = WideArea 3 = SubjectTracking
> 34.2 | LiveViewAFMode | int8u | [val >> 1 & 0x1] 0 = AF-C 1 = AF-F
> 35.1 | PlaybackMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min

## NikonCustom SettingsD4 Tags

Custom settings for the D4 and D4S.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | CustomSettingsBank | int8u | [val & 0x3] 0 = A 1 = B 2 = C 3 = D
> 1.1 | AF-CPrioritySelection | int8u | [val >> 6 & 0x3] 0 = Release 1 = Release + Focus 2 = Focus 3 = Focus + Release
> 1.2 | AF-SPrioritySelection | int8u | [val >> 5 & 0x1] 0 = Focus 1 = Release
> 1.3 | AFPointSelection | int8u | [val >> 4 & 0x1] 0 = 51 Points 1 = 11 Points
> 1.4 | FocusTrackingLockOn | int8u | [val & 0x7]
> 0 = Off 1 = 1 (Short) 2 = 2 |  | 3 = 3 (Normal) 4 = 4 5 = 5 (Long)
> 2.1 | AFActivation | int8u | [val >> 7 & 0x1] 0 = Shutter/AF-On 1 = AF-On Only
> 2.2 | FocusPointWrap | int8u | [val >> 3 & 0x1] 0 = No Wrap 1 = Wrap
> 4.1 | Pitch | int8u | [val >> 6 & 0x1] 0 = High 1 = Low
> 4.2 | NoMemoryCard | int8u | [val >> 5 & 0x1] 0 = Release Locked 1 = Enable Release
> 4.3 | GridDisplay | int8u | [val >> 1 & 0x1] 0 = On 1 = Off
> 5.1 | ShootingInfoDisplay | int8u | [val >> 6 & 0x3] 1 = Auto 2 = Manual (dark on light) 3 = Manual (light on dark)
> 5.2 | LCDIllumination | int8u | [val >> 5 & 0x1] 0 = Off 1 = On
> 5.3 | ScreenTips | int8u | [val >> 2 & 0x1] 0 = Off 1 = On
> 5.4 | Beep | int8u | [val & 0x3] 0 = Off 1 = Low 2 = Medium 3 = High
> 6.1 | ReverseIndicators | int8u | [val >> 7 & 0x1] 0 = + 0 - 1 = - 0 +
> 6.2 | RearDisplay | int8u | [val >> 6 & 0x1] 0 = ISO 1 = Exposures Remaining
> 6.3 | ViewfinderDisplay | int8u | [val >> 5 & 0x1] 0 = Frame Count 1 = Exposures Remaining
> 6.4 | CommandDialsReverseRotation | int8u | [val >> 3 & 0x3] 0 = No 1 = Shutter Speed & Aperture 2 = Exposure Compensation 3 = Exposure Compensation, Shutter Speed & Aperture
> 6.5 | EasyExposureCompensation | int8u | [val & 0x3] 0 = Off 1 = On 2 = On (auto reset)
> 7.1 | ExposureControlStepSize | int8u | [val >> 6 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 7.2 | ISOStepSize | int8u | [val >> 4 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 7.3 | ExposureCompStepSize | int8u | [val >> 2 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 8.1 | CenterWeightedAreaSize | int8u | [val >> 5 & 0x7] 0 = 8 mm 1 = 12 mm 2 = 15 mm 3 = 20 mm 4 = Average
> 8.2 | FineTuneOptMatrixMetering | int8u | [val & 0xf]
> 9.1 | FineTuneOptCenterWeighted | int8u | [val >> 4 & 0xf]
> 9.2 | FineTuneOptSpotMetering | int8u | [val & 0xf]
> 10.1 | MultiSelectorShootMode | int8u | [val >> 6 & 0x3] 0 = Select Center Focus Point (Reset) 2 = Preset Focus Point (Pre) 3 = Not Used (None)
> 10.2 | MultiSelectorPlaybackMode | int8u | [val >> 4 & 0x3] 0 = Thumbnail On/Off 1 = View Histograms 2 = Zoom On/Off 3 = Choose Folder
> 10.3 | MultiSelector | int8u | [val & 0x1] 0 = Do Nothing 1 = Reset Meter-off Delay
> 11.1 | ExposureDelayMode | int8u | [val >> 6 & 0x3] 0 = Off 1 = 1 s 2 = 2 s 3 = 3 s
> 11.2 | CHModeShootingSpeed | int8u | [val >> 4 & 0x1] 0 = 10 fps 1 = 11 fps
> 11.3 | CLModeShootingSpeed | int8u | [val & 0xf]
> 12 | MaxContinuousRelease | int8u |
> 13.1 | AutoBracketSet | int8u | [val >> 5 & 0x7] 0 = AE & Flash 1 = AE Only 2 = Flash Only 3 = WB Bracketing 4 = Active D-Lighting
> 13.2 | AutoBracketOrder | int8u | [val >> 4 & 0x1] 0 = 0,-,+ 1 = -,0,+
> 13.3 | AutoBracketModeM | int8u | [val >> 2 & 0x3] 0 = Flash/Speed 1 = Flash/Speed/Aperture 2 = Flash/Aperture 3 = Flash Only
> 14.1 | FuncButton | int8u | [val >> 3 & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 18 = My Menu 20 = Grid Display 21 = Disable Synchronized Release 22 = Remote Release Only 26 = Flash Disable/Enable
> 14.2 | FuncButtonPlusDials | int8u | [val & 0x7]
> 0 = None 1 = Choose Image Area (FX/DX/5:4) 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 6 = Shooting Bank Menu
> 15.1 | PreviewButton | int8u | [val >> 3 & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 18 = My Menu 20 = Grid Display 21 = Disable Synchronized Release 22 = Remote Release Only 26 = Flash Disable/Enable
> 15.2 | PreviewButtonPlusDials | int8u | [val & 0x7]
> 0 = None 1 = Choose Image Area (FX/DX/5:4) 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 6 = Shooting Bank Menu
> 16.1 | AssignBktButton | int8u | [val & 0x7] 0 = Auto Bracketing 1 = Multiple Exposure 2 = HDR (high dynamic range) 3 = None
> 18.1 | CommandDialsChangeMainSub | int8u | [val >> 5 & 0x7]
> 0 = Autofocus Off, Exposure Off 1 = Autofocus Off, Exposure On 2 = Autofocus Off, Exposure On (Mode A) 4 = Autofocus On, Exposure Off 5 = Autofocus On, Exposure On 6 = Autofocus On, Exposure On (Mode A)
> 18.2 | CommandDialsMenuAndPlayback | int8u | [val >> 3 & 0x3] 0 = On 1 = Off 2 = On (Image Review Excluded)
> 18.3 | CommandDialsApertureSetting | int8u | [val >> 2 & 0x1] 0 = Sub-command Dial 1 = Aperture Ring
> 18.4 | ShutterReleaseButtonAE-L | int8u | [val >> 1 & 0x1] 0 = Off 1 = On
> 18.5 | ReleaseButtonToUseDial | int8u | [val & 0x1] 0 = No 1 = Yes
> 19.1 | StandbyTimer | int8u | [val >> 4 & 0xf]
> 0 = 4 s 1 = 6 s 3 = 10 s 5 = 30 s |  | 6 = 1 min 7 = 5 min 8 = 10 min 9 = 30 min
> 20.1 | SelfTimerTime | int8u | [val >> 6 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 20.2 | SelfTimerShotCount | int8u | [val & 0xf]
> 20.3 | SelfTimerShotInterval | int8u | [val >> 4 & 0x3] 0 = 0.5 s 1 = 1 s 2 = 2 s 3 = 3 s
> 21.1 | ImageReviewMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 2 s 1 = 4 s 2 = 10 s 3 = 20 s |  | 4 = 1 min 5 = 5 min 6 = 10 min
> 21.2 | LiveViewMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 5 min 1 = 10 min 2 = 15 min |  | 3 = 20 min 4 = 30 min 5 = No Limit
> 22.1 | MenuMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 22.2 | ShootingInfoMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 23.1 | FlashSyncSpeed | int8u | [val >> 4 & 0xf]
> 1 = 1/250 s (auto FP) 2 = 1/250 s 3 = 1/200 s 4 = 1/160 s |  | 5 = 1/125 s 6 = 1/100 s 7 = 1/80 s 8 = 1/60 s
> 23.2 | FlashShutterSpeed | int8u | [val & 0xf]
> 0 = 1/60 s 1 = 1/30 s 2 = 1/15 s 3 = 1/8 s 4 = 1/4 s 5 = 1/2 s |  | 6 = 1 s 7 = 2 s 8 = 4 s 9 = 8 s 10 = 15 s 11 = 30 s
> 31.1 | ModelingFlash | int8u | [val >> 5 & 0x1] 0 = On 1 = Off
> 36.1 | PlaybackMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 37.1 | PlaybackZoom | int8u | [val & 0x1] 0 = Use Separate Zoom Buttons 1 = Use Either Zoom Button with Command Dial
> 38.1 | ShutterSpeedLock | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 38.2 | ApertureLock | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 38.3 | MovieShutterButton | int8u | [val >> 4 & 0x3] 0 = Take Photo 1 = Record Movies 2 = Live Frame Grab
> 38.4 | FlashExposureCompArea | int8u | [val >> 2 & 0x1] 0 = Entire frame 1 = Background only
> 41.1 | MovieFunctionButton | int8u | [val >> 4 & 0x7] 0 = None 1 = Power Aperture (open) 3 = Index Marking 4 = View Photo Shooting Info
> 41.2 | MoviePreviewButton | int8u | [val & 0x7] 0 = None 2 = Power Aperture (open) 3 = Index Marking 4 = View Photo Shooting Info
> 42.1 | VerticalMultiSelector | int8u | [val >> 5 & 0x3] 0 = Same as Multi-Selector with Info(U/D) & Playback(R/L) 1 = Same as Multi-Selector with Info(R/L) & Playback(U/D) 2 = Focus Point Selection
> 42.2 | VerticalFuncButton | int8u | [val & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 18 = My Menu 20 = Grid Display 26 = Flash Disable/Enable
> 43.1 | VerticalFuncButtonPlusDials | int8u | [val >> 4 & 0xf]
> 0 = None 1 = Choose Image Area (FX/DX/5:4) 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 6 = Shooting Bank Menu 7 = ISO Sensitivity 8 = Exposure Mode 9 = Exposure Compensation 10 = Metering
> 43.2 | AssignMovieRecordButton | int8u | [val & 0x7] 0 = None 1 = Choose Image Area (FX/DX/5:4) 2 = Shutter Speed & Aperture Lock 3 = ISO Sensitivity 4 = Shooting Bank Menu
> 46.1 | DynamicAreaAFDisplay | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 46.2 | AFPointIllumination | int8u | [val >> 5 & 0x3] 0 = Off 1 = On in Continuous Shooting Modes 2 = On During Manual Focusing 3 = On in Continuous Shooting and Manual Focusing
> 46.3 | StoreByOrientation | int8u | [val >> 3 & 0x3] 0 = Off 1 = Focus Point 2 = Focus Point and AF-area mode
> 46.4 | GroupAreaAFIllumination | int8u | [val >> 2 & 0x1] 0 = Squares 1 = Dots
> 46.5 | AFPointBrightness | int8u | [val & 0x3] 0 = Low 1 = Normal 2 = High 3 = Extra High
> 47.1 | AFOnButton | int8u | [val >> 4 & 0x7]
> 0 = AF On 1 = AE/AF Lock 2 = AE Lock Only 3 = AE Lock (reset on release) 4 = AE Lock (hold) 5 = AF Lock Only 6 = None
> 47.2 | VerticalAFOnButton | int8u | [val & 0x7]
> 0 = Same as AF On 1 = AF On 2 = AE/AF Lock 3 = AE Lock Only 4 = AE Lock (reset on release) 5 = AE Lock (hold) 6 = AF Lock Only 7 = None
> 48.1 | SubSelectorAssignment | int8u | [val >> 7 & 0x1] 0 = Focus Point Selection 1 = Same As Multi-selector
> 48.2 | MovieSubSelectorAssignment | int8u | [val & 0x7]
> 0 = None 1 = Index Marking 2 = AE/AF Lock 3 = AE Lock Only 4 = AE Lock (hold) 5 = AF Lock Only 6 = View Photo Shooting Info
> 49.1 | SubSelector | int8u | [val >> 3 & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 18 = My Menu 19 = Reset 20 = Grid Display 21 = Disable Synchronized Release 22 = Remote Release Only 23 = Preview 26 = Flash Disable/Enable
> 49.2 | SubSelectorPlusDials | int8u | [val & 0x7] 0 = None 1 = Choose Image Area (FX/DX/5:4) 2 = Shutter Speed & Aperture Lock 4 = Choose Non-CPU Lens Number 6 = Shooting Bank Menu
> 50.1 | MatrixMetering | int8u | (D4S only) [val >> 7 & 0x1] 0 = Face Detection On 1 = Face Detection Off
> 50.2 | LiveViewButtonOptions | int8u | (D4S only) [val >> 4 & 0x3] 0 = Enable 1 = Enable (standby time active) 2 = Disable
> 50.3 | AFModeRestrictions | int8u | (D4S only) [val & 0x3] 0 = Off 1 = AF-C 2 = AF-S
> 51.1 | LimitAFAreaModeSelection | int8u | (D4S only) [val >> 1 & 0x3f]
> 0x0 = No Restrictions Bit 0 = Auto-area Bit 1 = Group-area Bit 2 = 3D-tracking Bit 3 = Dynamic area (51 points) Bit 4 = Dynamic area (21 points) Bit 5 = Dynamic area (9 points)
> 52.1 | MovieFunctionButtonPlusDials | int8u | [val >> 4 & 0x1] 0 = None 1 = Choose Image Area
> 52.2 | MoviePreviewButtonPlusDials | int8u | [val & 0x1] 0 = None 1 = Choose Image Area
> 53.1 | MovieSubSelectorAssignmentPlusDials | int8u | [val >> 4 & 0x1] 0 = None 1 = Choose Image Area
> 54.1 | AssignRemoteFnButton | int8u | (D4S only) [val & 0x1f]
> 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 7 = AF Lock Only 8 = AF-On 16 = +NEF(RAW) 25 = Live View 26 = Flash Disable/Enable
> 55.1 | LensFocusFunctionButtons | int8u | (D4S only) [val & 0x3f]
> 3 = AE/AF Lock 4 = AE Lock Only 7 = AF Lock Only 21 = Disable Synchronized Release 22 = Remote Release Only 24 = Preset focus Point 26 = Flash Disable/Enable 32 = AF-Area Mode: Single-point AF 33 = AF-Area Mode: Dynamic-area AF (9 points) 34 = AF-Area Mode: Dynamic-area AF (21 points) 35 = AF-Area Mode: Dynamic-area AF (51 points) 36 = AF-Area Mode: Group-area AF 37 = AF-Area Mode: Auto area AF

## NikonCustom SettingsD5 Tags

Custom settings for the D5.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | CustomSettingsBank | int8u | [val & 0x3] 0 = A 1 = B 2 = C 3 = D
> 1.1 | AF-CPrioritySelection | int8u | [val >> 6 & 0x3] 0 = Release 1 = Release + Focus 2 = Focus 3 = Focus + Release
> 1.2 | AF-SPrioritySelection | int8u | [val >> 5 & 0x1] 0 = Focus 1 = Release
> 1.3 | NumberOfFocusPoints | int8u | [val >> 4 & 0x1] 0 = 55 Points 1 = 15 Points
> 1.4 | Three-DTrackingFaceDetection | int8u | [val >> 3 & 0x1] 0 = Off 1 = On
> 1.5 | BlockShotAFResponse | int8u | [val & 0x7]
> 2.1 | FocusPointWrap | int8u | [val >> 3 & 0x1] 0 = No Wrap 1 = Wrap
> 2.2 | AFPointBrightness | int8u | [val >> 1 & 0x3] 0 = Auto 1 = On 2 = Off
> 4.1 | ISODisplay | int8u | [val >> 3 & 0x1] 0 = Show ISO Sensitivity 1 = Show Frame Count
> 4.2 | GridDisplay | int8u | [val >> 1 & 0x1] 0 = On 1 = Off
> 5.1 | LCDIllumination | int8u | [val >> 5 & 0x1] 0 = Off 1 = On
> 5.2 | ElectronicFront-CurtainShutter | int8u | [val >> 3 & 0x1] 0 = Off 1 = On
> 6.1 | ReverseIndicators | int8u | [val >> 7 & 0x1] 0 = + 0 - 1 = - 0 +
> 6.2 | CommandDialsReverseRotation | int8u | [val >> 3 & 0x3] 0 = No 1 = Shutter Speed & Aperture 2 = Exposure Compensation 3 = Exposure Compensation, Shutter Speed & Aperture
> 6.3 | EasyExposureCompensation | int8u | [val & 0x3] 0 = Off 1 = On 2 = On (auto reset)
> 7.1 | ExposureControlStepSize | int8u | [val >> 6 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 7.2 | ISOStepSize | int8u | [val >> 4 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 7.3 | ExposureCompStepSize | int8u | [val >> 2 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 8.1 | CenterWeightedAreaSize | int8u | [val >> 5 & 0x7] 0 = 8 mm 1 = 12 mm 2 = 15 mm 3 = 20 mm 4 = Average
> 8.2 | FineTuneOptMatrixMetering | int8u | [val & 0xf]
> 9.1 | FineTuneOptCenterWeighted | int8u | [val >> 4 & 0xf]
> 9.2 | FineTuneOptSpotMetering | int8u | [val & 0xf]
> 10.1 | MultiSelectorShootMode | int8u | [val >> 5 & 0x7] 0 = Select Center Focus Point (Reset) 1 = Zoom On/Off 2 = Preset Focus Point (Pre) 4 = Not Used (None)
> 10.3 | MultiSelector | int8u | [val & 0x1] 0 = Do Nothing 1 = Reset Meter-off Delay
> 11.1 | ExposureDelayMode | int8u | [val >> 6 & 0x3] 0 = Off 1 = 1 s 2 = 2 s 3 = 3 s
> 11.2 | CLModeShootingSpeed | int8u | [val & 0xf]
> 12.1 | MaxContinuousRelease | int8u |
> 13.1 | AutoBracketOrder | int8u | [val >> 4 & 0x1] 0 = 0,-,+ 1 = -,0,+
> 13.2 | AutoBracketModeM | int8u | [val >> 2 & 0x3] 0 = Flash/Speed 1 = Flash/Speed/Aperture 2 = Flash/Aperture 3 = Flash Only
> 14.1 | Func1Button | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 19 = Grid Display 20 = My Menu 21 = Disable Synchronized Release 22 = Remote Release Only 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only)
> 15.1 | PreviewButton | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 19 = Grid Display 20 = My Menu 21 = Disable Synchronized Release 22 = Remote Release Only 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only)
> 16.1 | AssignBktButton | int8u | [val & 0x7] 0 = Auto Bracketing 1 = Multiple Exposure 2 = HDR (high dynamic range) 3 = None
> 18.1 | CommandDialsChangeMainSub | int8u | [val >> 5 & 0x7]
> 0 = Autofocus Off, Exposure Off 1 = Autofocus Off, Exposure On 2 = Autofocus Off, Exposure On (Mode A) 4 = Autofocus On, Exposure Off 5 = Autofocus On, Exposure On 6 = Autofocus On, Exposure On (Mode A)
> 18.2 | CommandDialsMenuAndPlayback | int8u | [val >> 3 & 0x3] 0 = On 1 = Off 2 = On (Image Review Excluded)
> 18.3 | CommandDialsApertureSetting | int8u | [val >> 2 & 0x1] 0 = Sub-command Dial 1 = Aperture Ring
> 18.4 | ReleaseButtonToUseDial | int8u | [val & 0x1] 0 = No 1 = Yes
> 19.1 | StandbyTimer | int8u | [val >> 4 & 0xf]
> 0 = 4 s 1 = 6 s 3 = 10 s |  | 5 = 30 s 6 = 1 min 7 = 5 min |  | 8 = 10 min 9 = 30 min 10 = No Limit
> 20.1 | SelfTimerTime | int8u | [val >> 6 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 20.2 | SelfTimerShotInterval | int8u | [val >> 4 & 0x3] 0 = 0.5 s 1 = 1 s 2 = 2 s 3 = 3 s
> 20.3 | SelfTimerShotCount | int8u | [val & 0xf]
> 21.1 | ImageReviewMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 2 s 1 = 4 s 3 = 10 s 4 = 20 s |  | 5 = 1 min 6 = 5 min 7 = 10 min
> 21.2 | LiveViewMonitorOffTime | int8u | [val >> 2 & 0x7]
> 1 = 5 min 2 = 10 min 3 = 15 min |  | 4 = 20 min 5 = 30 min 6 = No Limit
> 22.1 | MenuMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 2 = 10 s 4 = 20 s |  | 5 = 1 min 6 = 5 min 7 = 10 min
> 22.2 | ShootingInfoMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 2 = 10 s 4 = 20 s |  | 5 = 1 min 6 = 5 min 7 = 10 min
> 23.1 | FlashSyncSpeed | int8u | [val >> 4 & 0xf]
> 2 = 1/250 s (auto FP) 3 = 1/250 s 5 = 1/200 s 6 = 1/160 s |  | 7 = 1/125 s 8 = 1/100 s 9 = 1/80 s 10 = 1/60 s
> 23.2 | FlashShutterSpeed | int8u | [val & 0xf]
> 0 = 1/60 s 1 = 1/30 s 2 = 1/15 s 3 = 1/8 s 4 = 1/4 s 5 = 1/2 s |  | 6 = 1 s 7 = 2 s 8 = 4 s 9 = 8 s 10 = 15 s 11 = 30 s
> 31.1 | ModelingFlash | int8u | [val >> 5 & 0x1] 0 = On 1 = Off
> 36.1 | PlaybackMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 37.1 | MultiSelectorLiveView | int8u | [val >> 6 & 0x3] 0 = Reset 1 = Zoom 3 = Not Used
> 38.1 | ShutterSpeedLock | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 38.2 | ApertureLock | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 38.3 | MovieShutterButton | int8u | [val >> 4 & 0x1] 0 = Take Photo 1 = Record Movies
> 38.4 | FlashExposureCompArea | int8u | [val >> 2 & 0x1] 0 = Entire Frame 1 = Background Only
> 38.5 | AutoFlashISOSensitivity | int8u | [val >> 1 & 0x1] 0 = Subject and Background 1 = Subject Only
> 41.1 | MovieFunc1Button | int8u | [val >> 4 & 0xf] 0 = None 2 = Power Aperture (close) 3 = Index Marking 4 = View Photo Shooting Info 11 = Exposure Compensation -
> 41.2 | MoviePreviewButton | int8u | [val & 0xf] 0 = None 1 = Power Aperture (open) 3 = Index Marking 4 = View Photo Shooting Info 10 = Exposure Compensation +
> 42.1 | Func1ButtonPlusDials | int8u | [val & 0xf]
> 0 = None 1 = Choose Image Area 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 7 = Photo Shooting Menu Bank 8 = Exposure Delay Mode
> 43.1 | PreviewButtonPlusDials | int8u | [val & 0xf]
> 0 = None 1 = Choose Image Area 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 7 = Photo Shooting Menu Bank 8 = Exposure Delay Mode
> 45.1 | AssignMovieRecordButtonPlusDials | int8u | [val & 0xf] 0 = None 1 = Choose Image Area 2 = Shutter Speed & Aperture Lock 7 = Photo Shooting Menu Bank 11 = Exposure Mode
> 46.1 | FineTuneOptHighlightWeighted | int8u | [val & 0xf]
> 47.1 | DynamicAreaAFDisplay | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 47.2 | AFPointIllumination | int8u | [val >> 6 & 0x1] 0 = Off 1 = On During Manual Focusing
> 47.3 | StoreByOrientation | int8u | [val >> 3 & 0x3] 0 = Off 1 = Focus Point 2 = Focus Point and AF-area Mode
> 48.1 | MatrixMetering | int8u | [val >> 7 & 0x1] 0 = Face Detection On 1 = Face Detection Off
> 48.2 | LiveViewButtonOptions | int8u | [val >> 4 & 0x3] 0 = Enable 1 = Enable (Standby Timer Active) 2 = Disable
> 48.3 | AFModeRestrictions | int8u | [val & 0x3] 0 = No Restrictions 1 = AF-C 2 = AF-S
> 49.1 | LimitAFAreaModeSelection | int8u | [val >> 1 & 0x3f]
> 0x0 = No Restrictions Bit 0 = Auto-area Bit 1 = Group-area Bit 2 = 3D-tracking Bit 3 = Dynamic area (153 points) Bit 4 = Dynamic area (72 points) Bit 5 = Dynamic area (25 points)
> 52.1 | LensFocusFunctionButtons | int8u | [val & 0x3f] 3 = AE/AF Lock 4 = AE Lock Only 7 = AF Lock Only 8 = AF-On 24 = Preset Focus Point 26 = Flash Disable/Enable 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only)
> 66.1 | VerticalMultiSelector | int8u | [val & 0xff] 0x0 = Same as Multi-Selector with Info(U/D) & Playback(R/L) 0x8 = Same as Multi-Selector with Info(R/L) & Playback(U/D) 0x80 = Focus Point Selection
> 67.1 | VerticalFuncButton | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 18 = Reset Focus Point 19 = Grid Display 20 = My Menu 22 = Remote Release Only 23 = Preset Focus Point 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only) 54 = Highlight Active Focus Point
> 68.1 | VerticalFuncPlusDials | int8u | [val & 0xf]
> 0 = None 1 = Choose Image Area 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 7 = Photo Shooting Menu Bank 8 = Exposure Delay Mode 10 = ISO Sensitivity 11 = Exposure Mode 12 = Exposure Compensation 13 = Metering
> 70.1 | AF-OnButton | int8u | [val & 0x3f] 0 = None 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF)
> 71.1 | SubSelector | int8u | [val >> 7 & 0x1] 0 = Focus Point Selection 1 = Same as MultiSelector
> 72.1 | SubSelectorCenter | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 18 = Reset Focus Point 19 = Grid Display 20 = My Menu 22 = Remote Release Only 23 = Preset Focus Point 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only) 54 = Highlight Active Focus Point
> 73.1 | SubSelectorPlusDials | int8u | [val & 0xf] 0 = None 1 = Choose Image Area 2 = Shutter Speed & Aperture Lock 4 = Choose Non-CPU Lens Number 7 = Photo Shooting Menu Bank
> 74.1 | AssignMovieSubselector | int8u | [val >> 4 & 0xf]
> 0 = None 3 = Index Marking 4 = View Photo Shooting Info 5 = AE/AF Lock 6 = AE Lock (Only) 7 = AE Lock (Hold) 8 = AF Lock (Only)
> 75.1 | AssignMovieFunc1ButtonPlusDials | int8u | [val >> 4 & 0x1] 0 = None 1 = Choose Image Area
> 75.2 | AssignMoviePreviewButtonPlusDials | int8u | [val & 0x1] 0 = None 1 = Choose Image Area (DX/1.3x)
> 76.1 | AssignMovieSubselectorPlusDials | int8u | [val >> 4 & 0x1] 0 = None 1 = Choose Image Area
> 77.1 | SyncReleaseMode | int8u | [val >> 7 & 0x1] 0 = No Sync 1 = Sync
> 78.1 | Three-DTrackingWatchArea | int8u | [val >> 7 & 0x1] 0 = Wide 1 = Normal
> 78.2 | SubjectMotion | int8u | [val >> 5 & 0x3] 0 = Steady 1 = Middle 2 = Erratic
> 78.3 | AFActivation | int8u | [val >> 3 & 0x1] 0 = Shutter/AF-On 1 = AF-On Only
> 78.4 | ShutterReleaseButtonAE-L | int8u | [val & 0x3] 0 = Off 1 = On (Half Press) 2 = On (Burst Mode)
> 79.1 | VerticalAFOnButton | int8u | [val & 0x7f] 0 = None 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 100 = Same as AF-On
> 80.1 | Func2Button | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 19 = Grid Display 20 = My Menu 21 = Disable Synchronized Release 22 = Remote Release Only 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only)
> 81.1 | Func2ButtonPlusDials | int8u | [val & 0xf]
> 0 = None 1 = Choose Image Area 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 7 = Photo Shooting Menu Bank 8 = Exposure Delay Mode
> 82.1 | AssignMovieFunc2Button | int8u | [val >> 4 & 0x7] 0 = None 3 = Index Marking 4 = View Photo Shooting Info
> 83.1 | Func3Button | int8u | [val & 0x3] 0 = None 1 = Voice Memo 2 = Rating 3 = Connect To Network

## NikonCustom SettingsD500 Tags

Custom settings for the D500.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | CustomSettingsBank | int8u | [val & 0x3] 0 = A 1 = B 2 = C 3 = D
> 1.1 | AF-CPrioritySelection | int8u | [val >> 6 & 0x3] 0 = Release 1 = Release + Focus 2 = Focus 3 = Focus + Release
> 1.2 | AF-SPrioritySelection | int8u | [val >> 5 & 0x1] 0 = Focus 1 = Release
> 1.3 | NumberOfFocusPoints | int8u | [val >> 4 & 0x1] 0 = 55 Points 1 = 15 Points
> 1.4 | Three-DTrackingFaceDetection | int8u | [val >> 3 & 0x1] 0 = Off 1 = On
> 1.5 | BlockShotAFResponse | int8u | [val & 0x7]
> 2.1 | FocusPointWrap | int8u | [val >> 3 & 0x1] 0 = No Wrap 1 = Wrap
> 2.2 | AFPointBrightness | int8u | [val >> 1 & 0x3] 0 = Auto 1 = On 2 = Off
> 4.1 | ISODisplay | int8u | [val >> 3 & 0x1] 0 = Show ISO Sensitivity 1 = Show Frame Count
> 4.2 | GridDisplay | int8u | [val >> 1 & 0x1] 0 = On 1 = Off
> 5.1 | LCDIllumination | int8u | [val >> 5 & 0x1] 0 = Off 1 = On
> 5.2 | ElectronicFront-CurtainShutter | int8u | [val >> 3 & 0x1] 0 = Off 1 = On
> 6.1 | ReverseIndicators | int8u | [val >> 7 & 0x1] 0 = + 0 - 1 = - 0 +
> 6.2 | CommandDialsReverseRotation | int8u | [val >> 3 & 0x3] 0 = No 1 = Shutter Speed & Aperture 2 = Exposure Compensation 3 = Exposure Compensation, Shutter Speed & Aperture
> 6.3 | EasyExposureCompensation | int8u | [val & 0x3] 0 = Off 1 = On 2 = On (auto reset)
> 7.1 | ExposureControlStepSize | int8u | [val >> 6 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 7.2 | ISOStepSize | int8u | [val >> 4 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 7.3 | ExposureCompStepSize | int8u | [val >> 2 & 0x3] 0 = 1/3 EV 1 = 1/2 EV 2 = 1 EV
> 8.1 | CenterWeightedAreaSize | int8u | [val >> 5 & 0x7] 0 = 6 mm 1 = 8 mm 2 = 10 mm 3 = 13 mm 4 = Average
> 8.2 | FineTuneOptMatrixMetering | int8u | [val & 0xf]
> 9.1 | FineTuneOptCenterWeighted | int8u | [val >> 4 & 0xf]
> 9.2 | FineTuneOptSpotMetering | int8u | [val & 0xf]
> 10.1 | MultiSelectorShootMode | int8u | [val >> 5 & 0x7] 0 = Select Center Focus Point (Reset) 2 = Preset Focus Point (Pre) 3 = Highlight Active Focus Point 4 = Not Used (None)
> 10.2 | MultiSelectorPlaybackMode | int8u | [val >> 2 & 0x3] 0 = Thumbnail On/Off 1 = View Histograms 2 = Zoom On/Off 3 = Choose Folder
> 10.3 | MultiSelector | int8u | [val & 0x1] 0 = Do Nothing 1 = Reset Meter-off Delay
> 11.1 | ExposureDelayMode | int8u | [val >> 6 & 0x3] 0 = Off 1 = 1 s 2 = 2 s 3 = 3 s
> 11.2 | CLModeShootingSpeed | int8u | [val & 0xf]
> 12.1 | MaxContinuousRelease | int8u |
> 13.1 | AutoBracketOrder | int8u | [val >> 4 & 0x1] 0 = 0,-,+ 1 = -,0,+
> 13.2 | AutoBracketModeM | int8u | [val >> 2 & 0x3] 0 = Flash/Speed 1 = Flash/Speed/Aperture 2 = Flash/Aperture 3 = Flash Only
> 14.1 | Func1Button | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 19 = Grid Display 20 = My Menu 22 = Remote Release Only 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only)
> 15.1 | PreviewButton | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 19 = Grid Display 20 = My Menu 22 = Remote Release Only 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only)
> 16.1 | AssignBktButton | int8u | [val & 0x7] 0 = Auto Bracketing 1 = Multiple Exposure 2 = HDR (high dynamic range) 3 = None
> 18.1 | CommandDialsChangeMainSub | int8u | [val >> 5 & 0x7]
> 0 = Autofocus Off, Exposure Off 1 = Autofocus Off, Exposure On 2 = Autofocus Off, Exposure On (Mode A) 4 = Autofocus On, Exposure Off 5 = Autofocus On, Exposure On 6 = Autofocus On, Exposure On (Mode A)
> 18.2 | CommandDialsMenuAndPlayback | int8u | [val >> 3 & 0x3] 0 = On 1 = Off 2 = On (Image Review Excluded)
> 18.3 | CommandDialsApertureSetting | int8u | [val >> 2 & 0x1] 0 = Sub-command Dial 1 = Aperture Ring
> 18.4 | ReleaseButtonToUseDial | int8u | [val & 0x1] 0 = No 1 = Yes
> 19.1 | StandbyTimer | int8u | [val >> 4 & 0xf]
> 0 = 4 s 1 = 6 s 3 = 10 s |  | 5 = 30 s 6 = 1 min 7 = 5 min |  | 8 = 10 min 9 = 30 min 10 = No Limit
> 20.1 | SelfTimerTime | int8u | [val >> 6 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 20.2 | SelfTimerShotInterval | int8u | [val >> 4 & 0x3] 0 = 0.5 s 1 = 1 s 2 = 2 s 3 = 3 s
> 20.3 | SelfTimerShotCount | int8u | [val & 0xf]
> 21.1 | ImageReviewMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 2 s 1 = 4 s 3 = 10 s 4 = 20 s |  | 5 = 1 min 6 = 5 min 7 = 10 min
> 21.2 | LiveViewMonitorOffTime | int8u | [val >> 2 & 0x7]
> 1 = 5 min 2 = 10 min 3 = 15 min |  | 4 = 20 min 5 = 30 min 6 = No Limit
> 22.1 | MenuMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 2 = 10 s 4 = 20 s |  | 5 = 1 min 6 = 5 min 7 = 10 min
> 22.2 | ShootingInfoMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 2 = 10 s 4 = 20 s |  | 5 = 1 min 6 = 5 min 7 = 10 min
> 23.1 | FlashSyncSpeed | int8u | [val >> 4 & 0xf]
> 2 = 1/250 s (auto FP) 3 = 1/250 s 5 = 1/200 s 6 = 1/160 s |  | 7 = 1/125 s 8 = 1/100 s 9 = 1/80 s 10 = 1/60 s
> 23.2 | FlashShutterSpeed | int8u | [val & 0xf]
> 0 = 1/60 s 1 = 1/30 s 2 = 1/15 s 3 = 1/8 s 4 = 1/4 s 5 = 1/2 s |  | 6 = 1 s 7 = 2 s 8 = 4 s 9 = 8 s 10 = 15 s 11 = 30 s
> 31.1 | ModelingFlash | int8u | [val >> 5 & 0x1] 0 = On 1 = Off
> 36.1 | PlaybackMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 37.1 | MultiSelectorLiveView | int8u | [val >> 6 & 0x3] 0 = Reset 1 = Zoom 3 = Not Used
> 38.1 | ShutterSpeedLock | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 38.2 | ApertureLock | int8u | [val >> 6 & 0x1] 0 = Off 1 = On
> 38.3 | MovieShutterButton | int8u | [val >> 4 & 0x1] 0 = Take Photo 1 = Record Movies
> 38.4 | FlashExposureCompArea | int8u | [val >> 2 & 0x1] 0 = Entire Frame 1 = Background Only
> 38.5 | AutoFlashISOSensitivity | int8u | [val >> 1 & 0x1] 0 = Subject and Background 1 = Subject Only
> 41.1 | MovieFunc1Button | int8u | [val >> 4 & 0xf] 0 = None 2 = Power Aperture (close) 3 = Index Marking 4 = View Photo Shooting Info 11 = Exposure Compensation -
> 41.2 | MoviePreviewButton | int8u | [val & 0xf] 0 = None 1 = Power Aperture (open) 3 = Index Marking 4 = View Photo Shooting Info 10 = Exposure Compensation +
> 42.1 | Func1ButtonPlusDials | int8u | [val & 0xf]
> 0 = None 1 = Choose Image Area (DX/1.3x) 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 7 = Photo Shooting Menu Bank 8 = Exposure Delay Mode
> 43.1 | PreviewButtonPlusDials | int8u | [val & 0xf]
> 0 = None 1 = Choose Image Area (DX/1.3x) 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 7 = Photo Shooting Menu Bank 8 = Exposure Delay Mode
> 45.1 | AssignMovieRecordButtonPlusDials | int8u | [val & 0xf] 0 = None 1 = Choose Image Area (DX/1.3x) 2 = Shutter Speed & Aperture Lock 7 = Photo Shooting Menu Bank 11 = Exposure Mode
> 46.1 | FineTuneOptHighlightWeighted | int8u | [val & 0xf]
> 47.1 | DynamicAreaAFDisplay | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 47.2 | AFPointIllumination | int8u | [val >> 6 & 0x1] 0 = Off 1 = On During Manual Focusing
> 47.3 | StoreByOrientation | int8u | [val >> 3 & 0x3] 0 = Off 1 = Focus Point 2 = Focus Point and AF-area Mode
> 47.4 | GroupAreaAFIllumination | int8u | [val >> 2 & 0x1] 0 = Squares 1 = Dots
> 48.1 | MatrixMetering | int8u | [val >> 7 & 0x1] 0 = Face Detection On 1 = Face Detection Off
> 48.2 | LiveViewButtonOptions | int8u | [val >> 4 & 0x3] 0 = Enable 1 = Enable (Standby Timer Active) 2 = Disable
> 48.3 | AFModeRestrictions | int8u | [val & 0x3] 0 = No Restrictions 1 = AF-C 2 = AF-S
> 49.1 | LimitAFAreaModeSelection | int8u | [val >> 1 & 0x3f]
> 0x0 = No Restrictions Bit 0 = Auto-area Bit 1 = Group-area Bit 2 = 3D-tracking Bit 3 = Dynamic area (153 points) Bit 4 = Dynamic area (72 points) Bit 5 = Dynamic area (25 points)
> 52.1 | LensFocusFunctionButtons | int8u | [val & 0x3f] 3 = AE/AF Lock 4 = AE Lock Only 7 = AF Lock Only 8 = AF-On 24 = Preset Focus Point 26 = Flash Disable/Enable 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only)
> 66.1 | VerticalMultiSelector | int8u | [val & 0xff] 0x0 = Same as Multi-Selector with Info(U/D) & Playback(R/L) 0x8 = Same as Multi-Selector with Info(R/L) & Playback(U/D) 0x80 = Focus Point Selection
> 67.1 | AssignMB-D17FuncButton | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 18 = Reset Focus Point 19 = Grid Display 20 = My Menu 22 = Remote Release Only 23 = Preset Focus Point 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only) 54 = Highlight Active Focus Point
> 68.1 | AssignMB-D17FuncButtonPlusDials | int8u | [val & 0xf]
> 0 = None 1 = Choose Image Area (DX/1.3x) 2 = Shutter Speed & Aperture Lock 3 = One Step Speed / Aperture 4 = Choose Non-CPU Lens Number 5 = Active D-Lighting 7 = Photo Shooting Menu Bank 8 = Exposure Delay Mode 10 = ISO Sensitivity 11 = Exposure Mode 12 = Exposure Compensation 13 = Metering Mode
> 70.1 | AF-OnButton | int8u | [val & 0x3f] 0 = None 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF)
> 71.1 | SubSelector | int8u | [val >> 7 & 0x1] 0 = Focus Point Selection 1 = Same as MultiSelector
> 72.1 | SubSelectorCenter | int8u | [val & 0x3f] 0 = None 1 = Preview 2 = FV Lock 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 10 = Bracketing Burst 11 = Matrix Metering 12 = Center-weighted Metering 13 = Spot Metering 14 = Playback 15 = My Menu Top Item 16 = +NEF(RAW) 17 = Virtual Horizon 18 = Reset Focus Point 19 = Grid Display 20 = My Menu 22 = Remote Release Only 23 = Preset Focus Point 26 = Flash Disable/Enable 27 = Highlight-weighted Metering 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 49 = Sync Release (Master Only) 50 = Sync Release (Remote Only) 54 = Highlight Active Focus Point
> 73.1 | SubSelectorPlusDials | int8u | [val & 0xf] 0 = None 1 = Choose Image Area (DX/1.3x) 2 = Shutter Speed & Aperture Lock 4 = Choose Non-CPU Lens Number 7 = Photo Shooting Menu Bank
> 74.1 | AssignMovieSubselector | int8u | [val >> 4 & 0xf]
> 0 = None 3 = Index Marking 4 = View Photo Shooting Info 5 = AE/AF Lock 6 = AE Lock (Only) 7 = AE Lock (Hold) 8 = AF Lock (Only)
> 75.1 | AssignMovieFunc1ButtonPlusDials | int8u | [val >> 4 & 0x1] 0 = None 1 = Choose Image Area (DX/1.3x)
> 75.2 | AssignMoviePreviewButtonPlusDials | int8u | [val & 0x1] 0 = None 1 = Choose Image Area (DX/1.3x)
> 76.1 | AssignMovieSubselectorPlusDials | int8u | [val >> 4 & 0x1] 0 = None 1 = Choose Image Area (DX/1.3x)
> 77.1 | SyncReleaseMode | int8u | [val >> 7 & 0x1] 0 = No Sync 1 = Sync
> 78.1 | Three-DTrackingWatchArea | int8u | [val >> 7 & 0x1] 0 = Wide 1 = Normal
> 78.2 | SubjectMotion | int8u | [val >> 5 & 0x3] 0 = Steady 1 = Middle 2 = Erratic
> 78.3 | AFActivation | int8u | [val >> 3 & 0x1] 0 = Shutter/AF-On 1 = AF-On Only
> 78.4 | ShutterReleaseButtonAE-L | int8u | [val & 0x3] 0 = Off 1 = On (Half Press) 2 = On (Burst Mode)
> 79.1 | AssignMB-D17AF-OnButton | int8u | [val & 0x7f] 0 = None 3 = AE/AF Lock 4 = AE Lock Only 5 = AE Lock (reset on release) 6 = AE Lock (hold) 7 = AF Lock Only 8 = AF-On 36 = AF-Area Mode (Single) 37 = AF-Area Mode (Dynamic Area 25 Points) 38 = AF-Area Mode (Dynamic Area 72 Points) 39 = AF-Area Mode (Dynamic Area 152 Points) 40 = AF-Area Mode (Group Area AF) 41 = AF-Area Mode (Auto Area AF) 42 = AF-Area Mode + AF-On (Single) 43 = AF-Area Mode + AF-On (Dynamic Area 25 Points) 44 = AF-Area Mode + AF-On (Dynamic Area 72 Points) 45 = AF-Area Mode + AF-On (Dynamic Area 152 Points) 46 = AF-Area Mode + AF-On (Group Area AF) 47 = AF-Area Mode + AF-On (Auto Area AF) 100 = Same as Camera AF-On Button
> 80.1 | Func2Button | int8u | [val & 0x3f] 0 = None 15 = My Menu Top Item 20 = My Menu 55 = Rating
> 82.1 | AssignMovieFunc2Button | int8u | [val >> 4 & 0x7] 0 = None 3 = Index Marking 4 = View Photo Shooting Info

## NikonCustom SettingsD610 Tags

Custom settings for the D610.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | AF-CPrioritySelection | int8u | [val >> 7 & 0x1] 0 = Release 1 = Focus
> 0.2 | AF-SPrioritySelection | int8u | [val >> 5 & 0x1] 0 = Release 1 = Focus
> 0.3 | NumberOfFocusPoints | int8u | [val >> 4 & 0x1] 0 = 39 Points 1 = 11 Points
> 0.4 | FocusTrackingLockOn | int8u | [val & 0x7]
> 0 = Off 1 = 1 Short 2 = 2 |  | 3 = 3 Normal 4 = 4 5 = 5 Long
> 1.1 | FocusPointWrap | int8u | [val >> 3 & 0x1] 0 = No Wrap 1 = Wrap
> 1.2 | AFPointIllumination | int8u | [val >> 1 & 0x3] 0 = Auto 1 = On 2 = Off
> 1.3 | AFAssist | int8u | [val & 0x1] 0 = On 1 = Off
> 5.1 | EasyExposureCompensation | int8u | [val & 0x3] 0 = Off 1 = On 2 = On Auto Reset
> 6.1 | ExposureControlStep | int8u | [val >> 6 & 0x1] 0 = 1/3 EV 1 = 1/2 EV
> 6.2 | ISOSensitivityStep | int8u | [val >> 4 & 0x1] 0 = 1/3 EV 1 = 1/2 EV
> 7.1 | CenterWeightedAreaSize | int8u | [val >> 5 & 0x7] 0 = 8 mm 1 = 12 mm 2 = 15 mm 3 = 20 mm 4 = Average
> 7.2 | FineTuneOptMatrixMetering | int8u | [val & 0xf]
> 8.1 | FineTuneOptCenterWeighted | int8u | [val >> 4 & 0xf]
> 8.2 | FineTuneOptSpotMetering | int8u | [val & 0xf]
> 17.1 | ShutterReleaseButtonAE-L | int8u | [val >> 1 & 0x1] 0 = Off 1 = On
> 18.1 | StandbyTimer | int8u | [val >> 4 & 0xf]
> 0 = 4 s 1 = 6 s 2 = 10 s |  | 3 = 30 s 4 = 1 min 5 = 5 min |  | 6 = 10 min 7 = 30 min 8 = No Limit
> 18.2 | RemoteOnDuration | int8u | [val & 0x3] 0 = 1 min 1 = 5 min 2 = 10 min 3 = 20 min
> 19.1 | SelfTimerTime | int8u | [val >> 6 & 0x3] 0 = 2 s 1 = 5 s 2 = 10 s 3 = 20 s
> 19.2 | SelfTimerShotInterval | int8u | [val >> 4 & 0x3] 0 = 0.5 s 1 = 1 s 2 = 2 s 3 = 3 s
> 19.3 | SelfTimerShotCount | int8u | [val & 0xf]
> 20.1 | ImageReviewMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 2 s 1 = 4 s 2 = 10 s 3 = 20 s |  | 4 = 1 min 5 = 5 min 6 = 10 min
> 20.2 | LiveViewMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 5 min 1 = 10 min 2 = 15 min |  | 3 = 20 min 4 = 30 min 5 = No Limit
> 21.1 | MenuMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 21.2 | ShootingInfoMonitorOffTime | int8u | [val >> 2 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min
> 35.1 | PlaybackMonitorOffTime | int8u | [val >> 5 & 0x7]
> 0 = 4 s 1 = 10 s 2 = 20 s |  | 3 = 1 min 4 = 5 min 5 = 10 min

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Apr 12, 2019

<-- ExifTool Tag Names