## ExifTool Tag Names

The tables listed below give the names of all tags recognized by ExifTool.

> Tag Table Index
> JPEG EXIF IPTC XMP GPS GeoTiff ICC_Profile PrintIM Photoshop Apple Canon CanonCustom CanonVRD Casio FLIR FujiFilm GE HP JVC Kodak | Leaf Minolta Motorola Nikon NikonCustom NikonCapture Nintendo Olympus Panasonic Pentax PhaseOne Reconyx Sanyo Samsung Ricoh Sigma Sony SonyIDC Unknown DNG | CanonRaw KyoceraRaw MinoltaRaw PanasonicRaw SigmaRaw Lytro JFIF FlashPix MPF Stim Scalado Qualcomm APP12 AFCP DarwinCore FotoStation PhotoMechanic Microsoft GIMP MIE | Jpeg2000 GIF BMP PICT PNG MNG DjVu DPX OpenEXR MIFF PGF PSP PhotoCD Radiance PDF PostScript ID3 ITC Ogg Vorbis | FLAC Theora APE Audible MPC MPEG M2TS H264 QuickTime PLIST Matroska MOI MXF DV Flash Real RIFF AIFF ASF DICOM | HTML Palm Torrent EXE LNK Font VCard RSRC Rawzor ZIP RTF OOXML iWork Extra Composite Shortcuts MWG

Tag ID, Index# or Sequence is given in the first column of each table. A Tag ID is the computer-readable equivalent of a tag name, and is the identifier that is actually stored in the file. Index# refers to the location of a value when found at a fixed position within a data block (# is the multiplier for calculating a byte offset: 1, 2 or 4). Sequence gives the order of values for a serial data stream.

A Tag Name is the handle by which the information is accessed in ExifTool. In some instances, more than one name may correspond to a single tag ID. In these cases, the actual name used depends on the context in which the information is found. Case is not significant for tag names. A question mark (`?`) after a tag name indicates that the information is either not understood, not verified, or not very useful -- these tags are not extracted by ExifTool unless the Unknown (-u) option is enabled. Be aware that some tag names are different than the descriptions printed out by default when extracting information with exiftool. To see the tag names instead of the descriptions, use `exiftool -s`.

The Writable column indicates whether the tag is writable by ExifTool. Anything but an `N` in this column means the tag is writable. A `Y` indicates writable information that is either unformatted or written using the existing format. Other expressions give details about the information format, and vary depending on the general type of information. The format name may be followed by a number in square brackets to indicate the number of values written, or the number of characters in a fixed-length string (including a null terminator which is added if required).

A plus sign (`+`) after an entry in the Writable column indicates a "list" tag which supports multiple values and allows individual values to be added and deleted. A slash (`/`) indicates an "avoided" tag that is not created when writing if another same-named tag may be created instead. To write these tags, the group should be specified. A tilde (`~`) indicates a tag this is writable only when the print conversion is disabled (by setting PrintConv to 0, using the -n option, or suffixing the tag name with a `#` character). An exclamation point (`!`) indicates a tag that is considered unsafe to write under normal circumstances. These "unsafe" tags are not written unless specified explicitly (ie. wildcards and "all" may not be used), and care should be taken when editing them manually since they may affect the way an image is rendered. An asterisk (`*`) indicates a "protected" tag which is not writable directly, but is written automatically by ExifTool (often when a corresponding Composite or Extra tag is written). A colon (`:`) indicates a mandatory tag which may be added automatically when writing.

The HTML version of these tables also lists possible Values for discrete-valued tags, as well as Notes for some tags. The Values are listed as the computer-readable and human-readable values on the left and right hand side of an equals sign (`=`) respectively. The human-readable values are used by default when reading and writing, but the computer-readable values may be accessed by disabling the value conversion with the -n option on the command line, by setting the ValueConv option to 0 in the API, or or on a per-tag basis by adding a hash (`#`) after the tag name.

Note: If you are familiar with common meta-information tag names, you may find that some ExifTool tag names are different than expected. The usual reason for this is to make the tag names more consistent across different types of meta information. To determine a tag name, either consult this documentation or run `exiftool -s` on a file containing the information in question.

(This documentation is the result of years of research, testing and reverse engineering, and is the most complete metadata tag list available anywhere on the internet. It is provided not only for ExifTool users, but more importantly as a public service to help augment the collective knowledge, and is often used as a primary source of information in the development of other metadata software. Please help keep this documentation as accurate and complete as possible, and feed any new discoveries back to ExifTool. A big thanks to everyone who has helped with this so far!)

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Oct 30, 2015

<-- Back to ExifTool home page